{
    "content": "Gefest TestKl events description",
    "data": [
        {
            "addDesc": 0,
            "addDescUseDesc": 0,
            "bgColor": "Aqua",
            "code": 1,
            "desc": "Error: unable to create kernel object"
        },
        {
            "addDesc": 1,
            "addDescDesc": [
                {
                    "name": "task queue_EVENTs",
                    "value": 2
                },
                {
                    "name": "task queue_DriverLS_Event",
                    "value": 3
                },
                {
                    "name": "task queue_DriverModBus_Event",
                    "value": 4
                },
                {
                    "name": "task queue_DriverModBus_Event_2",
                    "value": 5
                },
                {
                    "name": "unknown error",
                    "value": 6
                }
            ],
            "addDescUseDesc": 1,
            "bgColor": "Aqua",
            "code": 2,
            "desc": "Error: message lost due to queue full"
        },
        {
            "addDesc": 1,
            "addDescDesc": [
                {
                    "name": "unknown error",
                    "value": 11
                },
                {
                    "name": "interrupt queue_EVENTs",
                    "value": 12
                },
                {
                    "name": "interrupt queue_DriverLS_Event",
                    "value": 13
                },
                {
                    "name": "interrupt queue_DriverModBus_Event",
                    "value": 14
                },
                {
                    "name": "interrupt queue_DriverModBus_Event_2",
                    "value": 15
                }
            ],
            "addDescUseDesc": 1,
            "bgColor": "Aqua",
            "code": 3,
            "desc": "Error: message lost due to queue full"
        },
        {
            "addDesc": 1,
            "addDescDesc": [
                {
                    "name": "task_InitLS (120 us)",
                    "value": 0
                }
            ],
            "addDescUseDesc": 1,
            "bgColor": "Aqua",
            "code": 4,
            "desc": "Error: semaphore not released"
        },
        {
            "addDesc": 1,
            "addDescDesc": [
                {
                    "name": "task_InitLS (right side, 20 ms)",
                    "value": 0
                }
            ],
            "addDescUseDesc": 1,
            "bgColor": "Aqua",
            "code": 5,
            "desc": "Error: semaphore not released"
        },
        {
            "addDesc": 1,
            "addDescDesc": [
                {
                    "name": "task_InitLS (0.7 ms)",
                    "value": 0
                }
            ],
            "addDescUseDesc": 1,
            "bgColor": "Aqua",
            "code": 6,
            "desc": "Error: semaphore not released"
        },
        {
            "addDesc": 1,
            "addDescDesc": [
                {
                    "name": "task_InitLS (120 us)",
                    "value": 0
                }
            ],
            "addDescUseDesc": 1,
            "bgColor": "Aqua",
            "code": 7,
            "desc": "Error: semaphore not released"
        },
        {
            "addDesc": 1,
            "addDescDesc": [
                {
                    "name": "task_InitLS (20 ms)",
                    "value": 0
                }
            ],
            "addDescUseDesc": 1,
            "bgColor": "Aqua",
            "code": 8,
            "desc": "Error: semaphore not released"
        },
        {
            "addDesc": 1,
            "addDescDesc": [
                {
                    "name": "task_InitLS (75 s)",
                    "value": 0
                }
            ],
            "addDescUseDesc": 1,
            "bgColor": "Aqua",
            "code": 9,
            "desc": "Error: semaphore not released"
        },
        {
            "addDesc": 1,
            "addDescDesc": [
                {
                    "name": "task_InitLS (left side, 20 ms)",
                    "value": 0
                }
            ],
            "addDescUseDesc": 1,
            "bgColor": "Aqua",
            "code": 10,
            "desc": "Error: semaphore not released"
        },
        {
            "addDesc": 1,
            "addDescDesc": [
                {
                    "name": "task_InitLS (left side, 75 s)",
                    "value": 0
                }
            ],
            "addDescUseDesc": 1,
            "bgColor": "Aqua",
            "code": 11,
            "desc": "Error: semaphore not released"
        },
        {
            "addDesc": 1,
            "addDescDesc": [
                {
                    "name": "task_InitLS (120 us, LME check)",
                    "value": 0
                }
            ],
            "addDescUseDesc": 1,
            "bgColor": "Aqua",
            "code": 12,
            "desc": "Error: semaphore not released"
        },
        {
            "addDesc": 1,
            "addDescDesc": [
                {
                    "name": "task_InitLS (50 ms)",
                    "value": 0
                }
            ],
            "addDescUseDesc": 1,
            "bgColor": "Aqua",
            "code": 13,
            "desc": "Error: semaphore not released"
        },
        {
            "addDesc": 1,
            "addDescDesc": [
                {
                    "name": "sDelayKZ_InitRight(Left)Dir",
                    "value": 0
                }
            ],
            "addDescUseDesc": 1,
            "bgColor": "Aqua",
            "code": 14,
            "desc": "Error: issuing available semaphore"
        },
        {
            "addDesc": 1,
            "addDescDesc": [
                {
                    "name": "sDelayInitLS",
                    "value": 0
                }
            ],
            "addDescUseDesc": 1,
            "bgColor": "Aqua",
            "code": 15,
            "desc": "Error: issuing available semaphore"
        },
        {
            "addDesc": 0,
            "addDescUseDesc": 0,
            "bgColor": "Aqua",
            "code": 16,
            "desc": "Error: OS stack overflow"
        },
        {
            "addDesc": 1,
            "addDescDesc": [
                {
                    "name": "FLASH_IRQHandler()",
                    "value": 0
                }
            ],
            "addDescUseDesc": 1,
            "bgColor": "Aqua",
            "code": 17,
            "desc": "Error: issuing available semaphore"
        },
        {
            "addDesc": 1,
            "addDescDesc": [
                {
                    "name": "flash_erase_page() \\ flash_write()",
                    "value": 0
                }
            ],
            "addDescUseDesc": 1,
            "bgColor": "Aqua",
            "code": 18,
            "desc": "Error: semaphore delay"
        },
        {
            "addDesc": 0,
            "addDescUseDesc": 0,
            "bgColor": "Aqua",
            "code": 19,
            "desc": "ModBus error - LC events not transm."
        },
        {
            "addDesc": 0,
            "addDescUseDesc": 0,
            "bgColor": "Aqua",
            "code": 20,
            "desc": "ModBus er. - no num. of events in buf."
        },
        {
            "addDesc": 1,
            "addDescDesc": [
                {
                    "name": "ADC data transfer error",
                    "value": 1
                },
                {
                    "name": "UART data transfer error",
                    "value": 4
                }
            ],
            "addDescUseDesc": 1,
            "bgColor": "Aqua",
            "code": 21,
            "desc": "DMA channel error"
        },
        {
            "addDesc": 1,
            "addDescPostfix": "elem.",
            "addDescUseDesc": 0,
            "bgColor": "Aqua",
            "code": 22,
            "desc": "Number of elements in overflowed queue"
        },
        {
            "addDesc": 1,
            "addDescPostfix": "unused elem.",
            "addDescUseDesc": 0,
            "bgColor": "Aqua",
            "code": 23,
            "desc": "Number of elements in overflowed queue"
        },
        {
            "addDesc": 0,
            "addDescUseDesc": 0,
            "bgColor": "Aqua",
            "code": 32,
            "desc": "Error: timer semaphore on delay 75 s"
        },
        {
            "addDesc": 1,
            "addDescDesc": [
                {
                    "name": "direct connection of ACL",
                    "value": 0
                }
            ],
            "addDescUseDesc": 1,
            "bgColor": "#ffd500",
            "code": 33,
            "desc": "LC initialization interrupted"
        },
        {
            "addDesc": 1,
            "addDescDesc": [
                {
                    "name": "there is an AD with reverse connection",
                    "value": 0
                }
            ],
            "addDescUseDesc": 1,
            "bgColor": "#ffd500",
            "code": 34,
            "desc": "Initialization complete"
        },
        {
            "addDesc": 1,
            "addDescDesc": [
                {
                    "name": "SC on left side",
                    "value": 1
                },
                {
                    "name": "SC on right side",
                    "value": 2
                },
                {
                    "name": "SC on right and left sides",
                    "value": 3
                },
                {
                    "name": "error in semaphores",
                    "value": 4
                },
                {
                    "name": "right LME signal when U from left side",
                    "value": 5
                },
                {
                    "name": "left LME signal when U from right side",
                    "value": 6
                },
                {
                    "name": "signal from LME when U from other side",
                    "value": 7
                },
                {
                    "name": "no signal from left LME",
                    "value": 8
                },
                {
                    "name": "no signal from right LME",
                    "value": 9
                },
                {
                    "name": "no signals from both LME",
                    "value": 10
                },
                {
                    "name": "in 75 s semaph. is used (left side ON)",
                    "value": 11
                },
                {
                    "name": "in 75 s semaph. is avail. (left side)",
                    "value": 12
                },
                {
                    "name": "in 75 s semaph.is used (right side ON)",
                    "value": 13
                },
                {
                    "name": "ACL SC on right\\left (both sides ON)",
                    "value": 14
                },
                {
                    "name": "SC of ACL or AD reverse connection",
                    "value": 15
                },
                {
                    "name": "unknown error",
                    "value": 16
                }
            ],
            "addDescUseDesc": 1,
            "bgColor": "#ffd500",
            "code": 35,
            "desc": "LC initialization interrupted"
        },
        {
            "addDesc": 1,
            "addDescDesc": [
                {
                    "name": "unknown error",
                    "value": 0
                }
            ],
            "addDescUseDesc": 1,
            "bgColor": "#ffd500",
            "code": 36,
            "desc": "LC initialization interrupted"
        },
        {
            "addDesc": 0,
            "addDescUseDesc": 0,
            "bgColor": "#fff9c3",
            "code": 39,
            "desc": "Response from disabled address"
        },
        {
            "addDesc": 1,
            "addDescDesc": [
                {
                    "name": "FHD-S, SMM up to ver. 3 or higher",
                    "value": 1
                },
                {
                    "name": "FSD up to version 6 or higher",
                    "value": 2
                }
            ],
            "addDescUseDesc": 1,
            "bgColor": "#fff9c3",
            "code": 40,
            "desc": "Firmware needs to be updated"
        },
        {
            "addDesc": 1,
            "addDescDesc": [
                {
                    "name": "AD incorrect polarity connection",
                    "value": 0
                }
            ],
            "addDescUseDesc": 1,
            "bgColor": "#fff9c3",
            "code": 41,
            "desc": "ACL fault, LC re-initialization"
        },
        {
            "addDesc": 0,
            "addDescUseDesc": 0,
            "bgColor": "Gold",
            "code": 51,
            "desc": "ACL is shorted on the left side"
        },
        {
            "addDesc": 0,
            "addDescUseDesc": 0,
            "bgColor": "Gold",
            "code": 52,
            "desc": "ACL is shorted on the right side"
        },
        {
            "addDesc": 0,
            "addDescUseDesc": 0,
            "bgColor": "Gold",
            "code": 53,
            "desc": "ACL is open"
        },
        {
            "addDesc": 0,
            "addDescUseDesc": 0,
            "bgColor": "Gold",
            "code": 54,
            "desc": "ACL is shorted"
        },
        {
            "addDesc": 0,
            "addDescUseDesc": 0,
            "bgColor": "Gold",
            "code": 55,
            "desc": "ACL is shorted behind the AD"
        },
        {
            "addDesc": 1,
            "addDescDesc": [
                {
                    "name": "contact bounce",
                    "value": 1
                }
            ],
            "addDescUseDesc": 1,
            "code": 56,
            "desc": "ACL short circuit location not found"
        },
        {
            "addDesc": 0,
            "addDescUseDesc": 0,
            "code": 57,
            "desc": "ACL fault location not found"
        },
        {
            "addDesc": 1,
            "addDescDesc": [
                {
                    "name": "f_Err_DlitD_Small \\ f_Err_DlitD_Big",
                    "value": 0
                }
            ],
            "addDescUseDesc": 1,
            "code": 58,
            "desc": "Data duration error (from AD)"
        },
        {
            "addDesc": 1,
            "addDescDesc": [
                {
                    "name": "f_Err_Time",
                    "value": 0
                }
            ],
            "addDescUseDesc": 1,
            "code": 59,
            "desc": "Timeout error (from AD)"
        },
        {
            "addDesc": 1,
            "addDescDesc": [
                {
                    "name": "f_Err_CRC",
                    "value": 0
                }
            ],
            "addDescUseDesc": 1,
            "code": 60,
            "desc": "Parity bit error (from AD)"
        },
        {
            "addDesc": 1,
            "addDescDesc": [
                {
                    "name": "out of range",
                    "value": 255
                }
            ],
            "addDescPrefix": "resistance (Ohm)",
            "addDescUseDesc": 1,
            "bgColor": "#fff9c3",
            "code": 61,
            "desc": "High resistance of ACL. No charge"
        },
        {
            "addDesc": 1,
            "addDescPostfix": "mA",
            "addDescPrefix": "response current",
            "addDescUseDesc": 0,
            "bgColor": "#fff9c3",
            "code": 62,
            "desc": "Low AD curr. (below 35/27mA for SB/DB)"
        },
        {
            "addDesc": 1,
            "addDescDesc": [
                {
                    "name": "entry",
                    "value": 1
                },
                {
                    "name": "exit",
                    "value": 2
                },
                {
                    "name": "incorrect password",
                    "value": 3
                }
            ],
            "addDescUseDesc": 1,
            "bgColor": "#00ffff",
            "code": 63,
            "desc": "Service menu"
        },
        {
            "addDesc": 1,
            "addDescPrefix": "register no.",
            "addDescUseDesc": 0,
            "bgColor": "#00ffff",
            "code": 64,
            "desc": "Recording a constant in LC"
        },
        {
            "addDesc": 0,
            "addDescUseDesc": 0,
            "bgColor": "#fff9c3",
            "code": 71,
            "desc": "Early signal from right LME"
        },
        {
            "addDesc": 1,
            "addDescDesc": [
                {
                    "name": "after opening",
                    "value": 1
                },
                {
                    "name": "after was shorted",
                    "value": 2
                }
            ],
            "addDescUseDesc": 1,
            "bgColor": "#7fff00",
            "code": 72,
            "desc": "ACL is Ok"
        },
        {
            "addDesc": 0,
            "addDescUseDesc": 0,
            "bgColor": "#fff9c3",
            "code": 73,
            "desc": "Early signal from left LME"
        },
        {
            "addDesc": 0,
            "addDescUseDesc": 0,
            "bgColor": "#ffd500",
            "code": 74,
            "desc": "Left LME fault"
        },
        {
            "addDesc": 0,
            "addDescUseDesc": 0,
            "bgColor": "#ffd500",
            "code": 75,
            "desc": "Right LME fault"
        },
        {
            "addDesc": 1,
            "addDescDesc": [
                {
                    "name": "sDEVICE.f_DriverLS_IsOn=0",
                    "value": 0
                }
            ],
            "addDescUseDesc": 1,
            "bgColor": "#aa00ff",
            "code": 77,
            "desc": "Error: Transmitter driver blocked",
            "fgColor": "#ffffff"
        },
        {
            "addDesc": 0,
            "addDescUseDesc": 0,
            "bgColor": "#ffd500",
            "code": 78,
            "desc": "Low power supply voltage"
        },
        {
            "addDesc": 0,
            "addDescUseDesc": 0,
            "bgColor": "#7fff00",
            "code": 79,
            "desc": "Power supply voltage is Ok"
        },
        {
            "addDesc": 0,
            "addDescUseDesc": 0,
            "bgColor": "#ffd500",
            "code": 80,
            "desc": "Mains fault"
        },
        {
            "addDesc": 0,
            "addDescUseDesc": 0,
            "bgColor": "#ffd500",
            "code": 81,
            "desc": "Battery fault"
        },
        {
            "addDesc": 0,
            "addDescUseDesc": 0,
            "bgColor": "#7fff00",
            "code": 82,
            "desc": "Mains is Ok"
        },
        {
            "addDesc": 0,
            "addDescUseDesc": 0,
            "bgColor": "#7fff00",
            "code": 83,
            "desc": "Battery is Ok"
        },
        {
            "addDesc": 1,
            "addDescPostfix": "°C",
            "addDescPrefix": "Δt=",
            "addDescUseDesc": 0,
            "code": 84,
            "desc": "Temperature is above average"
        },
        {
            "addDesc": 0,
            "addDescUseDesc": 0,
            "bgColor": "#ffd500",
            "code": 85,
            "desc": "Case tamper"
        },
        {
            "addDesc": 0,
            "addDescUseDesc": 0,
            "bgColor": "#7fff00",
            "code": 86,
            "desc": "Case is Ok"
        },
        {
            "addDesc": 1,
            "addDescDesc": [
                {
                    "name": "table of types",
                    "value": 1
                },
                {
                    "name": "table of temperatures",
                    "value": 2
                },
                {
                    "name": "table of disablements",
                    "value": 3
                },
                {
                    "name": "table of AMM initial states",
                    "value": 4
                },
                {
                    "name": "table of RMM initial states",
                    "value": 5
                },
                {
                    "name": "table of thermal channel types",
                    "value": 6
                },
                {
                    "name": "table of types (from SW)",
                    "value": 11
                },
                {
                    "name": "table of temperatures (from SW)",
                    "value": 12
                },
                {
                    "name": "table of disablements (from SW)",
                    "value": 13
                },
                {
                    "name": "table of AMM initial states (from SW)",
                    "value": 14
                },
                {
                    "name": "table of RMM initial states (from SW)",
                    "value": 15
                },
                {
                    "name": "table of thermal chan. types (from SW)",
                    "value": 16
                }
            ],
            "addDescUseDesc": 1,
            "code": 87,
            "desc": "Configuration table deleted successf."
        },
        {
            "addDesc": 1,
            "addDescDesc": [
                {
                    "name": "table of types",
                    "value": 1
                },
                {
                    "name": "table of temperatures",
                    "value": 2
                },
                {
                    "name": "table of disablements",
                    "value": 3
                },
                {
                    "name": "table of AMM initial states",
                    "value": 4
                },
                {
                    "name": "table of RMM initial states",
                    "value": 5
                },
                {
                    "name": "table of disablements (from SW)",
                    "value": 31
                }
            ],
            "addDescUseDesc": 1,
            "bgColor": "#fff9c3",
            "code": 88,
            "desc": "Error deleting configuration table"
        },
        {
            "addDesc": 1,
            "addDescDesc": [
                {
                    "name": "sDelayDriverLS",
                    "value": 0
                }
            ],
            "addDescUseDesc": 1,
            "bgColor": "#aa00ff",
            "code": 89,
            "desc": "Timer error",
            "fgColor": "#ffffff"
        },
        {
            "addDesc": 1,
            "addDescUseDesc": 0,
            "bgColor": "#aa00ff",
            "code": 90,
            "desc": "Safety timer is disabled",
            "fgColor": "#ffffff"
        },
        {
            "addDesc": 1,
            "addDescUseDesc": 0,
            "bgColor": "#aa00ff",
            "code": 99,
            "desc": "Transmitter driver blocked",
            "fgColor": "#ffffff"
        },
        {
            "addDesc": 1,
            "addDescDesc": [
                {
                    "name": "Reset LCs",
                    "value": 1
                },
                {
                    "name": "ACL left side ON (from software)",
                    "value": 3
                },
                {
                    "name": "ACL right side ON (from software)",
                    "value": 4
                },
                {
                    "name": "ACL left side OFF (from software)",
                    "value": 5
                },
                {
                    "name": "ACL right side OFF (from software)",
                    "value": 6
                },
                {
                    "name": "OPEN relay \"Fault.\" (from software)",
                    "value": 7
                },
                {
                    "name": "CLOSE relay \"Active\" (from software)",
                    "value": 8
                },
                {
                    "name": "CLOSE relay \"Fire\" (from software)",
                    "value": 9
                },
                {
                    "name": "CLOSE relay \"Fault\" (from software)",
                    "value": 11
                },
                {
                    "name": "OPEN relay \"Active\" (from software)",
                    "value": 12
                },
                {
                    "name": "OPEN relay \"Fire\" (from software)",
                    "value": 13
                },
                {
                    "name": "Clear table of disablements",
                    "value": 14
                },
                {
                    "name": "Clear table of types",
                    "value": 15
                },
                {
                    "name": "Clear table of temperatures",
                    "value": 16
                },
                {
                    "name": "Clear table of AMM initial states",
                    "value": 17
                },
                {
                    "name": "Clear table of RMM initial states",
                    "value": 18
                },
                {
                    "name": "Clear all tables / Request W1 (FFD)",
                    "value": 19
                },
                {
                    "name": "Clear FHD types table / Req. W2 (FFD)",
                    "value": 20
                },
                {
                    "name": "Change ModBus addr. / Request W3 (FFD)",
                    "value": 21
                },
                {
                    "name": "Check FFD pyrosensor",
                    "value": 63
                },
                {
                    "name": "Ionistors charge ON",
                    "value": 64
                },
                {
                    "name": "Ionistors charge OFF",
                    "value": 65
                },
                {
                    "name": "EAS (sprinkler) heating ON",
                    "value": 66
                },
                {
                    "name": "EAS (sprinkler) heating OFF",
                    "value": 67
                },
                {
                    "name": "Red LED ON",
                    "value": 68
                },
                {
                    "name": "Red LED OFF",
                    "value": 69
                },
                {
                    "name": "Yellow LED ON",
                    "value": 70
                },
                {
                    "name": "Yellow LED OFF",
                    "value": 71
                },
                {
                    "name": "\"Test\" mode ON",
                    "value": 72
                },
                {
                    "name": "\"Test\" mode OFF",
                    "value": 73
                },
                {
                    "name": "CLOSE left isolator",
                    "value": 74
                },
                {
                    "name": "OPEN left isolator",
                    "value": 75
                },
                {
                    "name": "CLOSE right isolator",
                    "value": 76
                },
                {
                    "name": "OPEN right isolator",
                    "value": 77
                },
                {
                    "name": "Laser ON (FFD)",
                    "value": 78
                },
                {
                    "name": "Laser OFF (FFD)",
                    "value": 79
                },
                {
                    "name": "CLOSE relay 1 (RMM)",
                    "value": 81
                },
                {
                    "name": "CLOSE relay 2 (RMM)",
                    "value": 82
                },
                {
                    "name": "CLOSE relays 1, 2 (RMM)",
                    "value": 83
                },
                {
                    "name": "CLOSE relay 3 (RMM)",
                    "value": 84
                },
                {
                    "name": "CLOSE relays 1, 3 (RMM)",
                    "value": 85
                },
                {
                    "name": "CLOSE relays 2, 3 (RMM)",
                    "value": 86
                },
                {
                    "name": "CLOSE relays 1-3 (RMM)",
                    "value": 87
                },
                {
                    "name": "CLOSE relay 4 (RMM)",
                    "value": 88
                },
                {
                    "name": "CLOSE relays 1, 4 (RMM)",
                    "value": 89
                },
                {
                    "name": "CLOSE relays 2, 4 (RMM)",
                    "value": 90
                },
                {
                    "name": "CLOSE relays 1, 2, 4 (RMM)",
                    "value": 91
                },
                {
                    "name": "CLOSE relays 3, 4 (RMM)",
                    "value": 92
                },
                {
                    "name": "CLOSE relays 1, 3, 4 (RMM)",
                    "value": 93
                },
                {
                    "name": "CLOSE relays 2-4 (RMM)",
                    "value": 94
                },
                {
                    "name": "CLOSE relays 1-4 (RMM)",
                    "value": 95
                },
                {
                    "name": "ACL left side ON",
                    "value": 103
                },
                {
                    "name": "ACL right side ON",
                    "value": 104
                },
                {
                    "name": "ACL left side OFF",
                    "value": 105
                },
                {
                    "name": "ACL right side OFF",
                    "value": 106
                },
                {
                    "name": "OPEN relay \"Fault\"",
                    "value": 107
                },
                {
                    "name": "CLOSE relay \"Active\"",
                    "value": 108
                },
                {
                    "name": "CLOSE relay \"Fire\"",
                    "value": 109
                },
                {
                    "name": "CLOSE relay \"Fault\"",
                    "value": 111
                },
                {
                    "name": "OPEN relay \"Active\"",
                    "value": 112
                },
                {
                    "name": "OPEN relay \"Fire\" / relay 1 (RMM)",
                    "value": 113
                },
                {
                    "name": "OPEN relay 2 (RMM)",
                    "value": 114
                },
                {
                    "name": "OPEN relays 1, 2 (RMM)",
                    "value": 115
                },
                {
                    "name": "OPEN relay 3 (RMM)",
                    "value": 116
                },
                {
                    "name": "OPEN relays 1, 3 (RMM)",
                    "value": 117
                },
                {
                    "name": "OPEN relays 2, 3 (RMM)",
                    "value": 118
                },
                {
                    "name": "OPEN relays 1-3 (RMM)",
                    "value": 119
                },
                {
                    "name": "OPEN relay 4 (RMM)",
                    "value": 120
                },
                {
                    "name": "OPEN relays 1, 4 (RMM)",
                    "value": 121
                },
                {
                    "name": "OPEN relays 2, 4 (RMM)",
                    "value": 122
                },
                {
                    "name": "OPEN relays 1, 2, 4 (RMM)",
                    "value": 123
                },
                {
                    "name": "OPEN relays 3, 4 (RMM)",
                    "value": 124
                },
                {
                    "name": "OPEN relays 1, 3, 4 (RMM)",
                    "value": 125
                },
                {
                    "name": "OPEN relays 2-4 (RMM)",
                    "value": 126
                },
                {
                    "name": "OPEN relays 1-4 (RMM)",
                    "value": 127
                },
                {
                    "name": "Change AD address",
                    "value": 128
                },
                {
                    "name": "Record W1 limit (FFD)",
                    "value": 140
                },
                {
                    "name": "Record W2 limit (FFD)",
                    "value": 141
                },
                {
                    "name": "Record W3 limit (FFD)",
                    "value": 142
                }
            ],
            "addDescUseDesc": 1,
            "bgColor": "#00ffff",
            "code": 100,
            "desc": "Command received in command register"
        },
        {
            "addDesc": 1,
            "addDescDesc": [
                {
                    "name": "reset on command",
                    "value": 1
                },
                {
                    "name": "power reset",
                    "value": 2
                },
                {
                    "name": "reset by WatchDog timer",
                    "value": 3
                },
                {
                    "name": "another reason",
                    "value": 5
                }
            ],
            "addDescUseDesc": 1,
            "bgColor": "DeepSkyBlue",
            "code": 101,
            "desc": "LC initialization"
        },
        {
            "addDesc": 1,
            "addDescPrefix": "LC ver.",
            "addDescUseDesc": 0,
            "bgColor": "#7fff00",
            "code": 102,
            "desc": "LC initializ. completed successfully"
        },
        {
            "addDesc": 1,
            "addDescDesc": [
                {
                    "name": "open, short circuit or addr. 251",
                    "value": 0
                }
            ],
            "addDescUseDesc": 1,
            "bgColor": "#ffd500",
            "code": 103,
            "desc": "ACL initializ. completed incorrectly"
        },
        {
            "addDesc": 1,
            "addDescPostfix": "Ohm",
            "addDescPrefix": "ACL resistance -",
            "addDescUseDesc": 0,
            "bgColor": "#7fff00",
            "code": 104,
            "desc": "ACL initializ. completed successfully"
        },
        {
            "addDesc": 1,
            "addDescDesc": [
                {
                    "name": "SC, open, 251, AD reverse connection",
                    "value": 0
                }
            ],
            "addDescUseDesc": 1,
            "bgColor": "#ffd500",
            "code": 105,
            "desc": "Error during ACL initialization"
        },
        {
            "addDesc": 0,
            "addDescUseDesc": 0,
            "code": 106,
            "desc": "Left side of ACL is ON"
        },
        {
            "addDesc": 0,
            "addDescUseDesc": 0,
            "code": 107,
            "desc": "Left side of ACL is OFF"
        },
        {
            "addDesc": 0,
            "addDescUseDesc": 0,
            "code": 108,
            "desc": "Right side of ACL is ON"
        },
        {
            "addDesc": 0,
            "addDescUseDesc": 0,
            "code": 109,
            "desc": "Right side of ACL is OFF"
        },
        {
            "addDesc": 0,
            "addDescUseDesc": 0,
            "code": 110,
            "desc": "Signal received from right LME"
        },
        {
            "addDesc": 0,
            "addDescUseDesc": 0,
            "code": 111,
            "desc": "Signal received from left LME"
        },
        {
            "addDesc": 1,
            "addDescDesc": [
                {
                    "name": "ACL short circuit",
                    "value": 1
                },
                {
                    "name": "Short circuit on both sides",
                    "value": 2
                },
                {
                    "name": "multiple short circuits",
                    "value": 3
                }
            ],
            "addDescUseDesc": 1,
            "bgColor": "Magenta",
            "code": 112,
            "desc": "LC operation stopped",
            "fgColor": "#ffffff"
        },
        {
            "addDesc": 0,
            "addDescUseDesc": 0,
            "code": 113,
            "desc": "ACL Initializing from left side"
        },
        {
            "addDesc": 0,
            "addDescUseDesc": 0,
            "code": 114,
            "desc": "ACL Initializing from right side"
        },
        {
            "addDesc": 0,
            "addDescUseDesc": 0,
            "bgColor": "#00ffff",
            "code": 115,
            "desc": "ACL command buffer overflow"
        },
        {
            "addDesc": 1,
            "addDescUseDesc": 0,
            "bgColor": "#00ffff",
            "code": 116,
            "desc": "Mutex not released, command not sent"
        },
        {
            "addDesc": 1,
            "addDescDesc": [
                {
                    "name": "in recording function itself",
                    "value": 1
                },
                {
                    "name": "error writing settings",
                    "value": 2
                },
                {
                    "name": "writing table of temperatures",
                    "value": 3
                },
                {
                    "name": "writing table of disablements",
                    "value": 4
                },
                {
                    "name": "writing table of types",
                    "value": 5
                },
                {
                    "name": "writing preamble",
                    "value": 6
                },
                {
                    "name": "table of AMM initial states",
                    "value": 7
                },
                {
                    "name": "table of RMM initial states",
                    "value": 8
                },
                {
                    "name": "table of thermal channel types",
                    "value": 9
                },
                {
                    "name": "LC constant",
                    "value": 10
                }
            ],
            "addDescUseDesc": 1,
            "bgColor": "#aa00ff",
            "code": 117,
            "desc": "FLASH write error",
            "fgColor": "#ffffff"
        },
        {
            "addDesc": 1,
            "addDescDesc": [
                {
                    "name": "table of temperatures",
                    "value": 1
                },
                {
                    "name": "table of disablements",
                    "value": 2
                },
                {
                    "name": "table of types",
                    "value": 3
                },
                {
                    "name": "table of AMM initial states",
                    "value": 5
                },
                {
                    "name": "table of RMM initial states",
                    "value": 6
                },
                {
                    "name": "table of thermal channel types",
                    "value": 7
                }
            ],
            "addDescUseDesc": 1,
            "code": 118,
            "desc": "Configuration written successfully"
        },
        {
            "addDesc": 1,
            "addDescDesc": [
                {
                    "name": "Polling",
                    "value": 0
                },
                {
                    "name": "Request AD type",
                    "value": 1
                },
                {
                    "name": "Request ionitors voltage",
                    "value": 2
                },
                {
                    "name": "Request sprinkler resistance",
                    "value": 3
                },
                {
                    "name": "Request U of lower ionistor",
                    "value": 5
                },
                {
                    "name": "Request U of middle ionistor",
                    "value": 6
                },
                {
                    "name": "Request U of upper ionistor",
                    "value": 7
                },
                {
                    "name": "Request processor type",
                    "value": 15
                },
                {
                    "name": "Request main power supply U (_MC_)",
                    "value": 16
                },
                {
                    "name": "Request backup power supply U (_MC_)",
                    "value": 17
                },
                {
                    "name": "Request drive power supply U (_MC_)",
                    "value": 18
                },
                {
                    "name": "Request W1 Limit (FFD)",
                    "value": 19
                },
                {
                    "name": "Request W2 Limit (FFD)",
                    "value": 20
                },
                {
                    "name": "Request W3 Limit (FFD)",
                    "value": 21
                },
                {
                    "name": "Request MCU2 type and FW version",
                    "value": 22
                },
                {
                    "name": "Check FFD pyrosensor",
                    "value": 63
                },
                {
                    "name": "Ionistors charge ON",
                    "value": 64
                },
                {
                    "name": "Ionistors charge OFF",
                    "value": 65
                },
                {
                    "name": "EAS (sprinkler) heating ON",
                    "value": 66
                },
                {
                    "name": "EAS (sprinkler) heating OFF",
                    "value": 67
                },
                {
                    "name": "Red LED ON",
                    "value": 68
                },
                {
                    "name": "Red LED OFF",
                    "value": 69
                },
                {
                    "name": "Yellow LED ON",
                    "value": 70
                },
                {
                    "name": "Yellow LED OFF",
                    "value": 71
                },
                {
                    "name": "\"Test\" mode ON",
                    "value": 72
                },
                {
                    "name": "\"Test\" mode OFF",
                    "value": 73
                },
                {
                    "name": "CLOSE left isolator",
                    "value": 74
                },
                {
                    "name": "OPEN left isolator",
                    "value": 75
                },
                {
                    "name": "CLOSE right isolator",
                    "value": 76
                },
                {
                    "name": "OPEN right isolator",
                    "value": 77
                },
                {
                    "name": "Laser ON (FFD)",
                    "value": 78
                },
                {
                    "name": "Laser OFF (FFD)",
                    "value": 79
                },
                {
                    "name": "CLOSE relay (RMM)",
                    "value": 80
                },
                {
                    "name": "ALC (AMM) in direct polarity mode",
                    "value": 96
                },
                {
                    "name": "ALC (AMM) in direct mode + flashing",
                    "value": 97
                },
                {
                    "name": "ALC (AMM) in reverse polarity mode",
                    "value": 98
                },
                {
                    "name": "ALC (AMM) in reverse mode + flashing",
                    "value": 99
                },
                {
                    "name": "Discharge resistor ON",
                    "value": 100
                },
                {
                    "name": "Discharge resistor OFF",
                    "value": 101
                },
                {
                    "name": "Photopath test",
                    "value": 102
                },
                {
                    "name": "OFF all relay (_MC_)",
                    "value": 106
                },
                {
                    "name": "ON relay K1 (_MC_)",
                    "value": 107
                },
                {
                    "name": "ON relay K2 (_MC_)",
                    "value": 108
                },
                {
                    "name": "OPEN relay (RMM)",
                    "value": 112
                },
                {
                    "name": "Change AD address",
                    "value": 128
                },
                {
                    "name": "Record W1 limit (FFD)",
                    "value": 140
                },
                {
                    "name": "Record W2 limit (FFD)",
                    "value": 141
                },
                {
                    "name": "Record W3 limit (FFD)",
                    "value": 142
                }
            ],
            "addDescUseDesc": 1,
            "bgColor": "#00ffff",
            "code": 119,
            "desc": "Command for AD (from LC keyboard)"
        },
        {
            "addDesc": 1,
            "addDescDesc": [
                {
                    "name": "no response",
                    "value": 0
                }
            ],
            "addDescUseDesc": 1,
            "bgColor": "#ffd500",
            "code": 120,
            "desc": "No connection with AD"
        },
        {
            "addDesc": 1,
            "addDescDesc": [
                {
                    "name": "reception errors",
                    "value": 0
                }
            ],
            "addDescUseDesc": 1,
            "bgColor": "#ffd500",
            "code": 121,
            "desc": "No connection with AD"
        },
        {
            "addDesc": 1,
            "addDescDesc": [
                {
                    "name": "after no connection",
                    "value": 0
                }
            ],
            "addDescUseDesc": 1,
            "bgColor": "#7fff00",
            "code": 122,
            "desc": "AD connection is Ok"
        },
        {
            "addDesc": 1,
            "addDescPrefix": "type",
            "addDescUseDesc": 0,
            "bgColor": "#fff9c3",
            "code": 123,
            "desc": "Unknown AD type"
        },
        {
            "addDesc": 1,
            "addDescDesc": [
                {
                    "name": "Polling",
                    "value": 0
                },
                {
                    "name": "Request AD type",
                    "value": 1
                },
                {
                    "name": "Request ionitors voltage",
                    "value": 2
                },
                {
                    "name": "Request sprinkler resistance",
                    "value": 3
                },
                {
                    "name": "Request U of lower ionistor",
                    "value": 5
                },
                {
                    "name": "Request U of middle ionistor",
                    "value": 6
                },
                {
                    "name": "Request U of upper ionistor",
                    "value": 7
                },
                {
                    "name": "Request processor type",
                    "value": 15
                },
                {
                    "name": "Request main power supply U (_MC_)",
                    "value": 16
                },
                {
                    "name": "Request backup power supply U (_MC_)",
                    "value": 17
                },
                {
                    "name": "Request drive power supply U (_MC_)",
                    "value": 18
                },
                {
                    "name": "Request W1 Limit (FFD)",
                    "value": 19
                },
                {
                    "name": "Request W2 Limit (FFD)",
                    "value": 20
                },
                {
                    "name": "Request W3 Limit (FFD)",
                    "value": 21
                },
                {
                    "name": "Check FFD pyrosensor",
                    "value": 63
                },
                {
                    "name": "Ionistors charge ON",
                    "value": 64
                },
                {
                    "name": "Ionistors charge OFF",
                    "value": 65
                },
                {
                    "name": "EAS (sprinkler) heating ON",
                    "value": 66
                },
                {
                    "name": "EAS (sprinkler) heating OFF",
                    "value": 67
                },
                {
                    "name": "Red LED ON",
                    "value": 68
                },
                {
                    "name": "Red LED OFF",
                    "value": 69
                },
                {
                    "name": "Yellow LED ON",
                    "value": 70
                },
                {
                    "name": "Yellow LED OFF",
                    "value": 71
                },
                {
                    "name": "\"Test\" mode ON",
                    "value": 72
                },
                {
                    "name": "\"Test\" mode OFF",
                    "value": 73
                },
                {
                    "name": "CLOSE left isolator",
                    "value": 74
                },
                {
                    "name": "OPEN left isolator",
                    "value": 75
                },
                {
                    "name": "CLOSE right isolator",
                    "value": 76
                },
                {
                    "name": "OPEN right isolator",
                    "value": 77
                },
                {
                    "name": "Laser ON (FFD)",
                    "value": 78
                },
                {
                    "name": "Laser OFF (FFD)",
                    "value": 79
                },
                {
                    "name": "CLOSE relay (RMM)",
                    "value": 80
                },
                {
                    "name": "ALC (AMM) in direct polarity mode",
                    "value": 96
                },
                {
                    "name": "ALC (AMM) in direct mode + flashing",
                    "value": 97
                },
                {
                    "name": "ALC (AMM) in reverse polarity mode",
                    "value": 98
                },
                {
                    "name": "ALC (AMM) in reverse mode + flashing",
                    "value": 99
                },
                {
                    "name": "Discharge resistor ON",
                    "value": 100
                },
                {
                    "name": "Discharge resistor OFF",
                    "value": 101
                },
                {
                    "name": "Photopath test",
                    "value": 102
                },
                {
                    "name": "OFF all relay (_MC_)",
                    "value": 106
                },
                {
                    "name": "ON relay K1 (_MC_)",
                    "value": 107
                },
                {
                    "name": "ON relay K2 (_MC_)",
                    "value": 108
                },
                {
                    "name": "OPEN relay (RMM)",
                    "value": 112
                },
                {
                    "name": "OPEN relay (RMM)",
                    "value": 113
                },
                {
                    "name": "OPEN relay 2 (RMM)",
                    "value": 114
                },
                {
                    "name": "OPEN relays 1, 2 (RMM)",
                    "value": 115
                },
                {
                    "name": "OPEN relay 3 (RMM)",
                    "value": 116
                },
                {
                    "name": "OPEN relays 1, 3 (RMM)",
                    "value": 117
                },
                {
                    "name": "OPEN relays 2, 3 (RMM)",
                    "value": 118
                },
                {
                    "name": "OPEN relays 1-3 (RMM)",
                    "value": 119
                },
                {
                    "name": "OPEN relay 4 (RMM)",
                    "value": 120
                },
                {
                    "name": "OPEN relays 1, 4 (RMM)",
                    "value": 121
                },
                {
                    "name": "OPEN relays 2, 4 (RMM)",
                    "value": 122
                },
                {
                    "name": "OPEN relays 1, 2, 4 (RMM)",
                    "value": 123
                },
                {
                    "name": "OPEN relays 3, 4 (RMM)",
                    "value": 124
                },
                {
                    "name": "OPEN relays 1, 3, 4 (RMM)",
                    "value": 125
                },
                {
                    "name": "OPEN relays 2-4 (RMM)",
                    "value": 126
                },
                {
                    "name": "OPEN relays 1-4 (RMM)",
                    "value": 127
                },
                {
                    "name": "Change AD address",
                    "value": 128
                },
                {
                    "name": "Record W1 limit (FFD)",
                    "value": 140
                },
                {
                    "name": "Record W2 limit (FFD)",
                    "value": 141
                },
                {
                    "name": "Record W3 limit (FFD)",
                    "value": 142
                }
            ],
            "addDescUseDesc": 1,
            "bgColor": "#fff9c3",
            "code": 124,
            "desc": "Failed to transmit a command"
        },
        {
            "addDesc": 0,
            "addDescUseDesc": 0,
            "bgColor": "#ffd500",
            "code": 125,
            "desc": "Double addr. (no charge of ionistors)"
        },
        {
            "addDesc": 0,
            "addDescUseDesc": 0,
            "bgColor": "#ffd500",
            "code": 126,
            "desc": "AD with address 251 detected"
        },
        {
            "addDesc": 1,
            "addDescDesc": [
                {
                    "name": "MCP",
                    "value": 1
                },
                {
                    "name": "FHD",
                    "value": 2
                },
                {
                    "name": "FHD-S",
                    "value": 3
                },
                {
                    "name": "FSD",
                    "value": 4
                },
                {
                    "name": "FFD",
                    "value": 5
                },
                {
                    "name": "FFD-S",
                    "value": 6
                },
                {
                    "name": "RAU",
                    "value": 7
                },
                {
                    "name": "IMM2",
                    "value": 8
                },
                {
                    "name": "IMM4",
                    "value": 9
                },
                {
                    "name": "RMM2",
                    "value": 10
                },
                {
                    "name": "RMM4",
                    "value": 11
                },
                {
                    "name": "MCP-B",
                    "value": 12
                },
                {
                    "name": "IRMM22",
                    "value": 13
                },
                {
                    "name": "IMM2A",
                    "value": 14
                },
                {
                    "name": "AMM(E)",
                    "value": 15
                },
                {
                    "name": "AMM(S)",
                    "value": 16
                },
                {
                    "name": "SMM",
                    "value": 17
                },
                {
                    "name": "_MC_",
                    "value": 18
                },
                {
                    "name": "_MCB_",
                    "value": 19
                },
                {
                    "name": "_MCBP_",
                    "value": 20
                },
                {
                    "name": "_MCR_",
                    "value": 21
                },
                {
                    "name": "_MCRS_",
                    "value": 22
                },
                {
                    "name": "FS/HD",
                    "value": 23
                },
                {
                    "name": "FS/HD-S",
                    "value": 24
                }
            ],
            "addDescPrefix": "type",
            "addDescUseDesc": 1,
            "bgColor": "#fff9c3",
            "code": 127,
            "desc": "Wrong AD type"
        },
        {
            "addDesc": 1,
            "addDescPrefix": "previous v.",
            "addDescUseDesc": 0,
            "bgColor": "#fff9c3",
            "code": 128,
            "desc": "AD software version has changed"
        },
        {
            "addDesc": 1,
            "addDescPrefix": "ADC",
            "addDescUseDesc": 0,
            "bgColor": "#ffd500",
            "code": 129,
            "desc": "Temperature sensor fault"
        },
        {
            "addDesc": 0,
            "addDescUseDesc": 0,
            "bgColor": "#00ffff",
            "code": 130,
            "desc": "ModBus message buffer overflow"
        },
        {
            "addDesc": 1,
            "addDescPrefix": "FHD current t,°C (for others - ADC)",
            "addDescUseDesc": 0,
            "bgColor": "#ff0000",
            "code": 131,
            "desc": "Fire",
            "fgColor": "White"
        },
        {
            "addDesc": 0,
            "addDescUseDesc": 0,
            "code": 132,
            "desc": "Table of disablements written success."
        },
        {
            "addDesc": 1,
            "addDescDesc": [
                {
                    "name": "table of temperatures",
                    "value": 1
                },
                {
                    "name": "table of disablements",
                    "value": 2
                },
                {
                    "name": "table of types",
                    "value": 3
                },
                {
                    "name": "preamble",
                    "value": 4
                },
                {
                    "name": "table of AMM initial states",
                    "value": 5
                },
                {
                    "name": "table of RMM initial states",
                    "value": 6
                },
                {
                    "name": "table of thermal channel types",
                    "value": 7
                }
            ],
            "addDescUseDesc": 1,
            "bgColor": "#aa00ff",
            "code": 133,
            "desc": "FLASH data verification error",
            "fgColor": "#ffffff"
        },
        {
            "addDesc": 0,
            "addDescUseDesc": 0,
            "bgColor": "#ffd500",
            "code": 134,
            "desc": "Ionistor fault (open or shorted)"
        },
        {
            "addDesc": 1,
            "addDescUseDesc": 0,
            "bgColor": "#7fff00",
            "code": 135,
            "desc": "Ionistor is Ok (after open or shorted)"
        },
        {
            "addDesc": 1,
            "addDescDesc": [
                {
                    "name": "0",
                    "value": 0
                },
                {
                    "name": "0,1",
                    "value": 1
                },
                {
                    "name": "0,2",
                    "value": 2
                },
                {
                    "name": "0,3",
                    "value": 3
                },
                {
                    "name": "0,4",
                    "value": 4
                },
                {
                    "name": "0,5",
                    "value": 5
                },
                {
                    "name": "0,6",
                    "value": 6
                },
                {
                    "name": "0,7",
                    "value": 7
                },
                {
                    "name": "0,8",
                    "value": 8
                },
                {
                    "name": "0,9",
                    "value": 9
                },
                {
                    "name": "1",
                    "value": 10
                },
                {
                    "name": "1,1",
                    "value": 11
                },
                {
                    "name": "1,2",
                    "value": 12
                },
                {
                    "name": "1,3",
                    "value": 13
                },
                {
                    "name": "1,4",
                    "value": 14
                },
                {
                    "name": "1,5",
                    "value": 15
                },
                {
                    "name": "1,6",
                    "value": 16
                },
                {
                    "name": "1,7",
                    "value": 17
                },
                {
                    "name": "1,8",
                    "value": 18
                },
                {
                    "name": "1,9",
                    "value": 19
                },
                {
                    "name": "2",
                    "value": 20
                },
                {
                    "name": "2,1",
                    "value": 21
                },
                {
                    "name": "2,2",
                    "value": 22
                },
                {
                    "name": "2,3",
                    "value": 23
                },
                {
                    "name": "2,4",
                    "value": 24
                },
                {
                    "name": "2,5",
                    "value": 25
                },
                {
                    "name": "2,6",
                    "value": 26
                },
                {
                    "name": "2,7",
                    "value": 27
                },
                {
                    "name": "2,8",
                    "value": 28
                },
                {
                    "name": "2,9",
                    "value": 29
                },
                {
                    "name": "3",
                    "value": 30
                },
                {
                    "name": "3,1",
                    "value": 31
                },
                {
                    "name": "3,2",
                    "value": 32
                },
                {
                    "name": "3,3",
                    "value": 33
                },
                {
                    "name": "3,4",
                    "value": 34
                },
                {
                    "name": "3,5",
                    "value": 35
                },
                {
                    "name": "3,6",
                    "value": 36
                },
                {
                    "name": "3,7",
                    "value": 37
                },
                {
                    "name": "3,8",
                    "value": 38
                },
                {
                    "name": "3,9",
                    "value": 39
                },
                {
                    "name": "4",
                    "value": 40
                },
                {
                    "name": "4,1",
                    "value": 41
                },
                {
                    "name": "4,2",
                    "value": 42
                },
                {
                    "name": "4,3",
                    "value": 43
                },
                {
                    "name": "4,4",
                    "value": 44
                },
                {
                    "name": "4,5",
                    "value": 45
                },
                {
                    "name": "4,6",
                    "value": 46
                },
                {
                    "name": "4,7",
                    "value": 47
                },
                {
                    "name": "4,8",
                    "value": 48
                },
                {
                    "name": "4,9",
                    "value": 49
                },
                {
                    "name": "5",
                    "value": 50
                },
                {
                    "name": "5,1",
                    "value": 51
                },
                {
                    "name": "5,2",
                    "value": 52
                },
                {
                    "name": "5,3",
                    "value": 53
                },
                {
                    "name": "5,4",
                    "value": 54
                },
                {
                    "name": "5,5",
                    "value": 55
                },
                {
                    "name": "5,6",
                    "value": 56
                },
                {
                    "name": "5,7",
                    "value": 57
                },
                {
                    "name": "5,8",
                    "value": 58
                },
                {
                    "name": "5,9",
                    "value": 59
                },
                {
                    "name": "6",
                    "value": 60
                },
                {
                    "name": "6,1",
                    "value": 61
                },
                {
                    "name": "6,2",
                    "value": 62
                },
                {
                    "name": "6,3",
                    "value": 63
                },
                {
                    "name": "6,4",
                    "value": 64
                },
                {
                    "name": "6,5",
                    "value": 65
                },
                {
                    "name": "6,6",
                    "value": 66
                },
                {
                    "name": "6,7",
                    "value": 67
                },
                {
                    "name": "6,8",
                    "value": 68
                },
                {
                    "name": "6,9",
                    "value": 69
                },
                {
                    "name": "7",
                    "value": 70
                },
                {
                    "name": "7,1",
                    "value": 71
                },
                {
                    "name": "7,2",
                    "value": 72
                },
                {
                    "name": "7,3",
                    "value": 73
                },
                {
                    "name": "7,4",
                    "value": 74
                },
                {
                    "name": "7,5",
                    "value": 75
                },
                {
                    "name": "7,6",
                    "value": 76
                },
                {
                    "name": "7,7",
                    "value": 77
                },
                {
                    "name": "7,8",
                    "value": 78
                },
                {
                    "name": "7,9",
                    "value": 79
                },
                {
                    "name": "8",
                    "value": 80
                },
                {
                    "name": "8,1",
                    "value": 81
                },
                {
                    "name": "8,2",
                    "value": 82
                },
                {
                    "name": "8,3",
                    "value": 83
                },
                {
                    "name": "8,4",
                    "value": 84
                },
                {
                    "name": "8,5",
                    "value": 85
                },
                {
                    "name": "8,6",
                    "value": 86
                },
                {
                    "name": "8,7",
                    "value": 87
                },
                {
                    "name": "8,8",
                    "value": 88
                },
                {
                    "name": "8,9",
                    "value": 89
                },
                {
                    "name": "9",
                    "value": 90
                },
                {
                    "name": "9,1",
                    "value": 91
                },
                {
                    "name": "9,2",
                    "value": 92
                },
                {
                    "name": "9,3",
                    "value": 93
                },
                {
                    "name": "9,4",
                    "value": 94
                },
                {
                    "name": "9,5",
                    "value": 95
                },
                {
                    "name": "9,6",
                    "value": 96
                },
                {
                    "name": "9,7",
                    "value": 97
                },
                {
                    "name": "9,8",
                    "value": 98
                },
                {
                    "name": "9,9",
                    "value": 99
                },
                {
                    "name": "10",
                    "value": 100
                },
                {
                    "name": "10,1",
                    "value": 101
                },
                {
                    "name": "10,2",
                    "value": 102
                },
                {
                    "name": "10,3",
                    "value": 103
                },
                {
                    "name": "10,4",
                    "value": 104
                },
                {
                    "name": "10,5",
                    "value": 105
                },
                {
                    "name": "10,6",
                    "value": 106
                },
                {
                    "name": "10,7",
                    "value": 107
                },
                {
                    "name": "10,8",
                    "value": 108
                },
                {
                    "name": "10,9",
                    "value": 109
                },
                {
                    "name": "11",
                    "value": 110
                },
                {
                    "name": "11,1",
                    "value": 111
                },
                {
                    "name": "11,2",
                    "value": 112
                },
                {
                    "name": "11,3",
                    "value": 113
                },
                {
                    "name": "11,4",
                    "value": 114
                },
                {
                    "name": "11,5",
                    "value": 115
                },
                {
                    "name": "11,6",
                    "value": 116
                },
                {
                    "name": "11,7",
                    "value": 117
                },
                {
                    "name": "11,8",
                    "value": 118
                },
                {
                    "name": "11,9",
                    "value": 119
                },
                {
                    "name": "12",
                    "value": 120
                },
                {
                    "name": "12,1",
                    "value": 121
                },
                {
                    "name": "12,2",
                    "value": 122
                },
                {
                    "name": "12,3",
                    "value": 123
                },
                {
                    "name": "12,4",
                    "value": 124
                },
                {
                    "name": "12,5",
                    "value": 125
                },
                {
                    "name": "12,6",
                    "value": 126
                },
                {
                    "name": "12,7",
                    "value": 127
                },
                {
                    "name": "12,8",
                    "value": 128
                },
                {
                    "name": "12,9",
                    "value": 129
                },
                {
                    "name": "13",
                    "value": 130
                },
                {
                    "name": "13,1",
                    "value": 131
                },
                {
                    "name": "13,2",
                    "value": 132
                },
                {
                    "name": "13,3",
                    "value": 133
                },
                {
                    "name": "13,4",
                    "value": 134
                },
                {
                    "name": "13,5",
                    "value": 135
                },
                {
                    "name": "13,6",
                    "value": 136
                },
                {
                    "name": "13,7",
                    "value": 137
                },
                {
                    "name": "13,8",
                    "value": 138
                },
                {
                    "name": "13,9",
                    "value": 139
                },
                {
                    "name": "14",
                    "value": 140
                },
                {
                    "name": "14,1",
                    "value": 141
                },
                {
                    "name": "14,2",
                    "value": 142
                },
                {
                    "name": "14,3",
                    "value": 143
                },
                {
                    "name": "14,4",
                    "value": 144
                },
                {
                    "name": "14,5",
                    "value": 145
                },
                {
                    "name": "14,6",
                    "value": 146
                },
                {
                    "name": "14,7",
                    "value": 147
                },
                {
                    "name": "14,8",
                    "value": 148
                },
                {
                    "name": "14,9",
                    "value": 149
                },
                {
                    "name": "15",
                    "value": 150
                }
            ],
            "addDescPostfix": "V",
            "addDescPrefix": "voltage",
            "addDescUseDesc": 1,
            "bgColor": "#ffffff",
            "code": 136,
            "desc": "Ionistors charging is ON"
        },
        {
            "addDesc": 0,
            "addDescUseDesc": 0,
            "bgColor": "#ffd500",
            "code": 137,
            "desc": "Sprinkler fault (open or shorted)"
        },
        {
            "addDesc": 0,
            "addDescUseDesc": 0,
            "bgColor": "#ff0000",
            "code": 138,
            "desc": "EAS (sprinkler) heating ON",
            "fgColor": "#ffffff"
        },
        {
            "addDesc": 0,
            "addDescUseDesc": 0,
            "code": 139,
            "desc": "EAS (sprinkler) heating OFF"
        },
        {
            "addDesc": 1,
            "addDescPrefix": "new address",
            "addDescUseDesc": 0,
            "code": 140,
            "desc": "AD address successfully set"
        },
        {
            "addDesc": 1,
            "addDescUseDesc": 0,
            "bgColor": "#fff9c3",
            "code": 141,
            "desc": "Error: wrong address set in AD"
        },
        {
            "addDesc": 0,
            "addDescUseDesc": 0,
            "bgColor": "#ffffff",
            "code": 142,
            "desc": "IMM input contact is closed"
        },
        {
            "addDesc": 0,
            "addDescUseDesc": 0,
            "bgColor": "#ffd500",
            "code": 143,
            "desc": "IMM input open"
        },
        {
            "addDesc": 0,
            "addDescUseDesc": 0,
            "bgColor": "#ffd500",
            "code": 144,
            "desc": "IMM input is shorted"
        },
        {
            "addDesc": 0,
            "addDescUseDesc": 0,
            "bgColor": "#7fff00",
            "code": 145,
            "desc": "LC is Ok"
        },
        {
            "addDesc": 1,
            "addDescDesc": [
                {
                    "name": "0",
                    "value": 0
                },
                {
                    "name": "0,1",
                    "value": 1
                },
                {
                    "name": "0,2",
                    "value": 2
                },
                {
                    "name": "0,3",
                    "value": 3
                },
                {
                    "name": "0,4",
                    "value": 4
                },
                {
                    "name": "0,5",
                    "value": 5
                },
                {
                    "name": "0,6",
                    "value": 6
                },
                {
                    "name": "0,7",
                    "value": 7
                },
                {
                    "name": "0,8",
                    "value": 8
                },
                {
                    "name": "0,9",
                    "value": 9
                },
                {
                    "name": "1",
                    "value": 10
                },
                {
                    "name": "1,1",
                    "value": 11
                },
                {
                    "name": "1,2",
                    "value": 12
                },
                {
                    "name": "1,3",
                    "value": 13
                },
                {
                    "name": "1,4",
                    "value": 14
                },
                {
                    "name": "1,5",
                    "value": 15
                },
                {
                    "name": "1,6",
                    "value": 16
                },
                {
                    "name": "1,7",
                    "value": 17
                },
                {
                    "name": "1,8",
                    "value": 18
                },
                {
                    "name": "1,9",
                    "value": 19
                },
                {
                    "name": "2",
                    "value": 20
                },
                {
                    "name": "2,1",
                    "value": 21
                },
                {
                    "name": "2,2",
                    "value": 22
                },
                {
                    "name": "2,3",
                    "value": 23
                },
                {
                    "name": "2,4",
                    "value": 24
                },
                {
                    "name": "2,5",
                    "value": 25
                },
                {
                    "name": "2,6",
                    "value": 26
                },
                {
                    "name": "2,7",
                    "value": 27
                },
                {
                    "name": "2,8",
                    "value": 28
                },
                {
                    "name": "2,9",
                    "value": 29
                },
                {
                    "name": "3",
                    "value": 30
                },
                {
                    "name": "3,1",
                    "value": 31
                },
                {
                    "name": "3,2",
                    "value": 32
                },
                {
                    "name": "3,3",
                    "value": 33
                },
                {
                    "name": "3,4",
                    "value": 34
                },
                {
                    "name": "3,5",
                    "value": 35
                },
                {
                    "name": "3,6",
                    "value": 36
                },
                {
                    "name": "3,7",
                    "value": 37
                },
                {
                    "name": "3,8",
                    "value": 38
                },
                {
                    "name": "3,9",
                    "value": 39
                },
                {
                    "name": "4",
                    "value": 40
                },
                {
                    "name": "4,1",
                    "value": 41
                },
                {
                    "name": "4,2",
                    "value": 42
                },
                {
                    "name": "4,3",
                    "value": 43
                },
                {
                    "name": "4,4",
                    "value": 44
                },
                {
                    "name": "4,5",
                    "value": 45
                },
                {
                    "name": "4,6",
                    "value": 46
                },
                {
                    "name": "4,7",
                    "value": 47
                },
                {
                    "name": "4,8",
                    "value": 48
                },
                {
                    "name": "4,9",
                    "value": 49
                },
                {
                    "name": "5",
                    "value": 50
                },
                {
                    "name": "5,1",
                    "value": 51
                },
                {
                    "name": "5,2",
                    "value": 52
                },
                {
                    "name": "5,3",
                    "value": 53
                },
                {
                    "name": "5,4",
                    "value": 54
                },
                {
                    "name": "5,5",
                    "value": 55
                },
                {
                    "name": "5,6",
                    "value": 56
                },
                {
                    "name": "5,7",
                    "value": 57
                },
                {
                    "name": "5,8",
                    "value": 58
                },
                {
                    "name": "5,9",
                    "value": 59
                },
                {
                    "name": "6",
                    "value": 60
                },
                {
                    "name": "6,1",
                    "value": 61
                },
                {
                    "name": "6,2",
                    "value": 62
                },
                {
                    "name": "6,3",
                    "value": 63
                },
                {
                    "name": "6,4",
                    "value": 64
                },
                {
                    "name": "6,5",
                    "value": 65
                },
                {
                    "name": "6,6",
                    "value": 66
                },
                {
                    "name": "6,7",
                    "value": 67
                },
                {
                    "name": "6,8",
                    "value": 68
                },
                {
                    "name": "6,9",
                    "value": 69
                },
                {
                    "name": "7",
                    "value": 70
                },
                {
                    "name": "7,1",
                    "value": 71
                },
                {
                    "name": "7,2",
                    "value": 72
                },
                {
                    "name": "7,3",
                    "value": 73
                },
                {
                    "name": "7,4",
                    "value": 74
                },
                {
                    "name": "7,5",
                    "value": 75
                },
                {
                    "name": "7,6",
                    "value": 76
                },
                {
                    "name": "7,7",
                    "value": 77
                },
                {
                    "name": "7,8",
                    "value": 78
                },
                {
                    "name": "7,9",
                    "value": 79
                },
                {
                    "name": "8",
                    "value": 80
                },
                {
                    "name": "8,1",
                    "value": 81
                },
                {
                    "name": "8,2",
                    "value": 82
                },
                {
                    "name": "8,3",
                    "value": 83
                },
                {
                    "name": "8,4",
                    "value": 84
                },
                {
                    "name": "8,5",
                    "value": 85
                },
                {
                    "name": "8,6",
                    "value": 86
                },
                {
                    "name": "8,7",
                    "value": 87
                },
                {
                    "name": "8,8",
                    "value": 88
                },
                {
                    "name": "8,9",
                    "value": 89
                },
                {
                    "name": "9",
                    "value": 90
                },
                {
                    "name": "9,1",
                    "value": 91
                },
                {
                    "name": "9,2",
                    "value": 92
                },
                {
                    "name": "9,3",
                    "value": 93
                },
                {
                    "name": "9,4",
                    "value": 94
                },
                {
                    "name": "9,5",
                    "value": 95
                },
                {
                    "name": "9,6",
                    "value": 96
                },
                {
                    "name": "9,7",
                    "value": 97
                },
                {
                    "name": "9,8",
                    "value": 98
                },
                {
                    "name": "9,9",
                    "value": 99
                },
                {
                    "name": "10",
                    "value": 100
                },
                {
                    "name": "10,1",
                    "value": 101
                },
                {
                    "name": "10,2",
                    "value": 102
                },
                {
                    "name": "10,3",
                    "value": 103
                },
                {
                    "name": "10,4",
                    "value": 104
                },
                {
                    "name": "10,5",
                    "value": 105
                },
                {
                    "name": "10,6",
                    "value": 106
                },
                {
                    "name": "10,7",
                    "value": 107
                },
                {
                    "name": "10,8",
                    "value": 108
                },
                {
                    "name": "10,9",
                    "value": 109
                },
                {
                    "name": "11",
                    "value": 110
                },
                {
                    "name": "11,1",
                    "value": 111
                },
                {
                    "name": "11,2",
                    "value": 112
                },
                {
                    "name": "11,3",
                    "value": 113
                },
                {
                    "name": "11,4",
                    "value": 114
                },
                {
                    "name": "11,5",
                    "value": 115
                },
                {
                    "name": "11,6",
                    "value": 116
                },
                {
                    "name": "11,7",
                    "value": 117
                },
                {
                    "name": "11,8",
                    "value": 118
                },
                {
                    "name": "11,9",
                    "value": 119
                },
                {
                    "name": "12",
                    "value": 120
                },
                {
                    "name": "12,1",
                    "value": 121
                },
                {
                    "name": "12,2",
                    "value": 122
                },
                {
                    "name": "12,3",
                    "value": 123
                },
                {
                    "name": "12,4",
                    "value": 124
                },
                {
                    "name": "12,5",
                    "value": 125
                },
                {
                    "name": "12,6",
                    "value": 126
                },
                {
                    "name": "12,7",
                    "value": 127
                },
                {
                    "name": "12,8",
                    "value": 128
                },
                {
                    "name": "12,9",
                    "value": 129
                },
                {
                    "name": "13",
                    "value": 130
                },
                {
                    "name": "13,1",
                    "value": 131
                },
                {
                    "name": "13,2",
                    "value": 132
                },
                {
                    "name": "13,3",
                    "value": 133
                },
                {
                    "name": "13,4",
                    "value": 134
                },
                {
                    "name": "13,5",
                    "value": 135
                },
                {
                    "name": "13,6",
                    "value": 136
                },
                {
                    "name": "13,7",
                    "value": 137
                },
                {
                    "name": "13,8",
                    "value": 138
                },
                {
                    "name": "13,9",
                    "value": 139
                },
                {
                    "name": "14",
                    "value": 140
                },
                {
                    "name": "14,1",
                    "value": 141
                },
                {
                    "name": "14,2",
                    "value": 142
                },
                {
                    "name": "14,3",
                    "value": 143
                },
                {
                    "name": "14,4",
                    "value": 144
                },
                {
                    "name": "14,5",
                    "value": 145
                },
                {
                    "name": "14,6",
                    "value": 146
                },
                {
                    "name": "14,7",
                    "value": 147
                },
                {
                    "name": "14,8",
                    "value": 148
                },
                {
                    "name": "14,9",
                    "value": 149
                },
                {
                    "name": "15",
                    "value": 150
                }
            ],
            "addDescPostfix": "V",
            "addDescPrefix": "voltage",
            "addDescUseDesc": 1,
            "bgColor": "#ffd500",
            "code": 146,
            "desc": "Ionistors are discharged"
        },
        {
            "addDesc": 1,
            "addDescDesc": [
                {
                    "name": "0",
                    "value": 0
                },
                {
                    "name": "0,1",
                    "value": 1
                },
                {
                    "name": "0,2",
                    "value": 2
                },
                {
                    "name": "0,3",
                    "value": 3
                },
                {
                    "name": "0,4",
                    "value": 4
                },
                {
                    "name": "0,5",
                    "value": 5
                },
                {
                    "name": "0,6",
                    "value": 6
                },
                {
                    "name": "0,7",
                    "value": 7
                },
                {
                    "name": "0,8",
                    "value": 8
                },
                {
                    "name": "0,9",
                    "value": 9
                },
                {
                    "name": "1",
                    "value": 10
                },
                {
                    "name": "1,1",
                    "value": 11
                },
                {
                    "name": "1,2",
                    "value": 12
                },
                {
                    "name": "1,3",
                    "value": 13
                },
                {
                    "name": "1,4",
                    "value": 14
                },
                {
                    "name": "1,5",
                    "value": 15
                },
                {
                    "name": "1,6",
                    "value": 16
                },
                {
                    "name": "1,7",
                    "value": 17
                },
                {
                    "name": "1,8",
                    "value": 18
                },
                {
                    "name": "1,9",
                    "value": 19
                },
                {
                    "name": "2",
                    "value": 20
                },
                {
                    "name": "2,1",
                    "value": 21
                },
                {
                    "name": "2,2",
                    "value": 22
                },
                {
                    "name": "2,3",
                    "value": 23
                },
                {
                    "name": "2,4",
                    "value": 24
                },
                {
                    "name": "2,5",
                    "value": 25
                },
                {
                    "name": "2,6",
                    "value": 26
                },
                {
                    "name": "2,7",
                    "value": 27
                },
                {
                    "name": "2,8",
                    "value": 28
                },
                {
                    "name": "2,9",
                    "value": 29
                },
                {
                    "name": "3",
                    "value": 30
                },
                {
                    "name": "3,1",
                    "value": 31
                },
                {
                    "name": "3,2",
                    "value": 32
                },
                {
                    "name": "3,3",
                    "value": 33
                },
                {
                    "name": "3,4",
                    "value": 34
                },
                {
                    "name": "3,5",
                    "value": 35
                },
                {
                    "name": "3,6",
                    "value": 36
                },
                {
                    "name": "3,7",
                    "value": 37
                },
                {
                    "name": "3,8",
                    "value": 38
                },
                {
                    "name": "3,9",
                    "value": 39
                },
                {
                    "name": "4",
                    "value": 40
                },
                {
                    "name": "4,1",
                    "value": 41
                },
                {
                    "name": "4,2",
                    "value": 42
                },
                {
                    "name": "4,3",
                    "value": 43
                },
                {
                    "name": "4,4",
                    "value": 44
                },
                {
                    "name": "4,5",
                    "value": 45
                },
                {
                    "name": "4,6",
                    "value": 46
                },
                {
                    "name": "4,7",
                    "value": 47
                },
                {
                    "name": "4,8",
                    "value": 48
                },
                {
                    "name": "4,9",
                    "value": 49
                },
                {
                    "name": "5",
                    "value": 50
                },
                {
                    "name": "5,1",
                    "value": 51
                },
                {
                    "name": "5,2",
                    "value": 52
                },
                {
                    "name": "5,3",
                    "value": 53
                },
                {
                    "name": "5,4",
                    "value": 54
                },
                {
                    "name": "5,5",
                    "value": 55
                },
                {
                    "name": "5,6",
                    "value": 56
                },
                {
                    "name": "5,7",
                    "value": 57
                },
                {
                    "name": "5,8",
                    "value": 58
                },
                {
                    "name": "5,9",
                    "value": 59
                },
                {
                    "name": "6",
                    "value": 60
                },
                {
                    "name": "6,1",
                    "value": 61
                },
                {
                    "name": "6,2",
                    "value": 62
                },
                {
                    "name": "6,3",
                    "value": 63
                },
                {
                    "name": "6,4",
                    "value": 64
                },
                {
                    "name": "6,5",
                    "value": 65
                },
                {
                    "name": "6,6",
                    "value": 66
                },
                {
                    "name": "6,7",
                    "value": 67
                },
                {
                    "name": "6,8",
                    "value": 68
                },
                {
                    "name": "6,9",
                    "value": 69
                },
                {
                    "name": "7",
                    "value": 70
                },
                {
                    "name": "7,1",
                    "value": 71
                },
                {
                    "name": "7,2",
                    "value": 72
                },
                {
                    "name": "7,3",
                    "value": 73
                },
                {
                    "name": "7,4",
                    "value": 74
                },
                {
                    "name": "7,5",
                    "value": 75
                },
                {
                    "name": "7,6",
                    "value": 76
                },
                {
                    "name": "7,7",
                    "value": 77
                },
                {
                    "name": "7,8",
                    "value": 78
                },
                {
                    "name": "7,9",
                    "value": 79
                },
                {
                    "name": "8",
                    "value": 80
                },
                {
                    "name": "8,1",
                    "value": 81
                },
                {
                    "name": "8,2",
                    "value": 82
                },
                {
                    "name": "8,3",
                    "value": 83
                },
                {
                    "name": "8,4",
                    "value": 84
                },
                {
                    "name": "8,5",
                    "value": 85
                },
                {
                    "name": "8,6",
                    "value": 86
                },
                {
                    "name": "8,7",
                    "value": 87
                },
                {
                    "name": "8,8",
                    "value": 88
                },
                {
                    "name": "8,9",
                    "value": 89
                },
                {
                    "name": "9",
                    "value": 90
                },
                {
                    "name": "9,1",
                    "value": 91
                },
                {
                    "name": "9,2",
                    "value": 92
                },
                {
                    "name": "9,3",
                    "value": 93
                },
                {
                    "name": "9,4",
                    "value": 94
                },
                {
                    "name": "9,5",
                    "value": 95
                },
                {
                    "name": "9,6",
                    "value": 96
                },
                {
                    "name": "9,7",
                    "value": 97
                },
                {
                    "name": "9,8",
                    "value": 98
                },
                {
                    "name": "9,9",
                    "value": 99
                },
                {
                    "name": "10",
                    "value": 100
                },
                {
                    "name": "10,1",
                    "value": 101
                },
                {
                    "name": "10,2",
                    "value": 102
                },
                {
                    "name": "10,3",
                    "value": 103
                },
                {
                    "name": "10,4",
                    "value": 104
                },
                {
                    "name": "10,5",
                    "value": 105
                },
                {
                    "name": "10,6",
                    "value": 106
                },
                {
                    "name": "10,7",
                    "value": 107
                },
                {
                    "name": "10,8",
                    "value": 108
                },
                {
                    "name": "10,9",
                    "value": 109
                },
                {
                    "name": "11",
                    "value": 110
                },
                {
                    "name": "11,1",
                    "value": 111
                },
                {
                    "name": "11,2",
                    "value": 112
                },
                {
                    "name": "11,3",
                    "value": 113
                },
                {
                    "name": "11,4",
                    "value": 114
                },
                {
                    "name": "11,5",
                    "value": 115
                },
                {
                    "name": "11,6",
                    "value": 116
                },
                {
                    "name": "11,7",
                    "value": 117
                },
                {
                    "name": "11,8",
                    "value": 118
                },
                {
                    "name": "11,9",
                    "value": 119
                },
                {
                    "name": "12",
                    "value": 120
                },
                {
                    "name": "12,1",
                    "value": 121
                },
                {
                    "name": "12,2",
                    "value": 122
                },
                {
                    "name": "12,3",
                    "value": 123
                },
                {
                    "name": "12,4",
                    "value": 124
                },
                {
                    "name": "12,5",
                    "value": 125
                },
                {
                    "name": "12,6",
                    "value": 126
                },
                {
                    "name": "12,7",
                    "value": 127
                },
                {
                    "name": "12,8",
                    "value": 128
                },
                {
                    "name": "12,9",
                    "value": 129
                },
                {
                    "name": "13",
                    "value": 130
                },
                {
                    "name": "13,1",
                    "value": 131
                },
                {
                    "name": "13,2",
                    "value": 132
                },
                {
                    "name": "13,3",
                    "value": 133
                },
                {
                    "name": "13,4",
                    "value": 134
                },
                {
                    "name": "13,5",
                    "value": 135
                },
                {
                    "name": "13,6",
                    "value": 136
                },
                {
                    "name": "13,7",
                    "value": 137
                },
                {
                    "name": "13,8",
                    "value": 138
                },
                {
                    "name": "13,9",
                    "value": 139
                },
                {
                    "name": "14",
                    "value": 140
                },
                {
                    "name": "14,1",
                    "value": 141
                },
                {
                    "name": "14,2",
                    "value": 142
                },
                {
                    "name": "14,3",
                    "value": 143
                },
                {
                    "name": "14,4",
                    "value": 144
                },
                {
                    "name": "14,5",
                    "value": 145
                },
                {
                    "name": "14,6",
                    "value": 146
                },
                {
                    "name": "14,7",
                    "value": 147
                },
                {
                    "name": "14,8",
                    "value": 148
                },
                {
                    "name": "14,9",
                    "value": 149
                },
                {
                    "name": "15",
                    "value": 150
                } 
            ],
            "addDescPostfix": "V",
            "addDescPrefix": "voltage",
            "addDescUseDesc": 1,
            "code": 147,
            "desc": "Ionistors charging is OFF"
        },
        {
            "addDesc": 0,
            "addDescUseDesc": 0,
            "bgColor": "#ff0000",
            "code": 148,
            "desc": "Sprinkler is open",
            "fgColor": "White"
        },
        {
            "addDesc": 0,
            "addDescUseDesc": 0,
            "code": 149,
            "desc": "Module output is OPEN"
        },
        {
            "addDesc": 0,
            "addDescUseDesc": 0,
            "bgColor": "#ffffff",
            "code": 150,
            "desc": "Module output is CLOSED"
        },
        {
            "addDesc": 1,
            "addDescDesc": [
                {
                    "name": "open or shorted",
                    "value": 0
                }
            ],
            "addDescUseDesc": 1,
            "bgColor": "#ffd500",
            "code": 151,
            "desc": "Optorelay fault (RMM output)"
        },
        {
            "addDesc": 1,
            "addDescDesc": [
                {
                    "name": "unspecified",
                    "value": 0
                }
            ],
            "addDescUseDesc": 1,
            "bgColor": "#ffd500",
            "code": 152,
            "desc": "Optorelay fault (RMM output)"
        },
        {
            "addDesc": 0,
            "addDescUseDesc": 0,
            "bgColor": "Red",
            "code": 153,
            "desc": "MCP button pressed",
            "fgColor": "#ffffff"
        },
        {
            "addDesc": 0,
            "addDescUseDesc": 0,
            "code": 154,
            "desc": "MCP button released"
        },
        {
            "addDesc": 0,
            "addDescUseDesc": 0,
            "bgColor": "Red",
            "code": 155,
            "desc": "RAU button pressed",
            "fgColor": "#ffffff"
        },
        {
            "addDesc": 1,
            "addDescDesc": [
                {
                    "name": "button pressed with closed lid",
                    "value": 0
                }
            ],
            "addDescUseDesc": 1,
            "bgColor": "#ffd500",
            "code": 156,
            "desc": "RAU failure"
        },
        {
            "addDesc": 0,
            "addDescUseDesc": 0,
            "code": 157,
            "desc": "RAU lid is open"
        },
        {
            "addDesc": 0,
            "addDescUseDesc": 0,
            "code": 158,
            "desc": "RAU lid is closed"
        },
        {
            "addDesc": 0,
            "addDescUseDesc": 0,
            "code": 159,
            "desc": "RAU button released"
        },
        {
            "addDesc": 1,
            "addDescDesc": [
                {
                    "name": "AD disable OFF",
                    "value": 0
                },
                {
                    "name": "AD disable ON",
                    "value": 1
                }
            ],
            "addDescUseDesc": 1,
            "bgColor": "#ffd500",
            "code": 160,
            "desc": "Changing the disablement state"
        },
        {
            "addDesc": 1,
            "addDescDesc": [
                {
                    "name": "0",
                    "value": 0
                },
                {
                    "name": "0,1",
                    "value": 1
                },
                {
                    "name": "0,2",
                    "value": 2
                },
                {
                    "name": "0,3",
                    "value": 3
                },
                {
                    "name": "0,4",
                    "value": 4
                },
                {
                    "name": "0,5",
                    "value": 5
                },
                {
                    "name": "0,6",
                    "value": 6
                },
                {
                    "name": "0,7",
                    "value": 7
                },
                {
                    "name": "0,8",
                    "value": 8
                },
                {
                    "name": "0,9",
                    "value": 9
                },
                {
                    "name": "1",
                    "value": 10
                },
                {
                    "name": "1,1",
                    "value": 11
                },
                {
                    "name": "1,2",
                    "value": 12
                },
                {
                    "name": "1,3",
                    "value": 13
                },
                {
                    "name": "1,4",
                    "value": 14
                },
                {
                    "name": "1,5",
                    "value": 15
                },
                {
                    "name": "1,6",
                    "value": 16
                },
                {
                    "name": "1,7",
                    "value": 17
                },
                {
                    "name": "1,8",
                    "value": 18
                },
                {
                    "name": "1,9",
                    "value": 19
                },
                {
                    "name": "2",
                    "value": 20
                },
                {
                    "name": "2,1",
                    "value": 21
                },
                {
                    "name": "2,2",
                    "value": 22
                },
                {
                    "name": "2,3",
                    "value": 23
                },
                {
                    "name": "2,4",
                    "value": 24
                },
                {
                    "name": "2,5",
                    "value": 25
                },
                {
                    "name": "2,6",
                    "value": 26
                },
                {
                    "name": "2,7",
                    "value": 27
                },
                {
                    "name": "2,8",
                    "value": 28
                },
                {
                    "name": "2,9",
                    "value": 29
                },
                {
                    "name": "3",
                    "value": 30
                },
                {
                    "name": "3,1",
                    "value": 31
                },
                {
                    "name": "3,2",
                    "value": 32
                },
                {
                    "name": "3,3",
                    "value": 33
                },
                {
                    "name": "3,4",
                    "value": 34
                },
                {
                    "name": "3,5",
                    "value": 35
                },
                {
                    "name": "3,6",
                    "value": 36
                },
                {
                    "name": "3,7",
                    "value": 37
                },
                {
                    "name": "3,8",
                    "value": 38
                },
                {
                    "name": "3,9",
                    "value": 39
                },
                {
                    "name": "4",
                    "value": 40
                },
                {
                    "name": "4,1",
                    "value": 41
                },
                {
                    "name": "4,2",
                    "value": 42
                },
                {
                    "name": "4,3",
                    "value": 43
                },
                {
                    "name": "4,4",
                    "value": 44
                },
                {
                    "name": "4,5",
                    "value": 45
                },
                {
                    "name": "4,6",
                    "value": 46
                },
                {
                    "name": "4,7",
                    "value": 47
                },
                {
                    "name": "4,8",
                    "value": 48
                },
                {
                    "name": "4,9",
                    "value": 49
                },
                {
                    "name": "5",
                    "value": 50
                },
                {
                    "name": "5,1",
                    "value": 51
                },
                {
                    "name": "5,2",
                    "value": 52
                },
                {
                    "name": "5,3",
                    "value": 53
                },
                {
                    "name": "5,4",
                    "value": 54
                },
                {
                    "name": "5,5",
                    "value": 55
                },
                {
                    "name": "5,6",
                    "value": 56
                },
                {
                    "name": "5,7",
                    "value": 57
                },
                {
                    "name": "5,8",
                    "value": 58
                },
                {
                    "name": "5,9",
                    "value": 59
                },
                {
                    "name": "6",
                    "value": 60
                },
                {
                    "name": "6,1",
                    "value": 61
                },
                {
                    "name": "6,2",
                    "value": 62
                },
                {
                    "name": "6,3",
                    "value": 63
                },
                {
                    "name": "6,4",
                    "value": 64
                },
                {
                    "name": "6,5",
                    "value": 65
                },
                {
                    "name": "6,6",
                    "value": 66
                },
                {
                    "name": "6,7",
                    "value": 67
                },
                {
                    "name": "6,8",
                    "value": 68
                },
                {
                    "name": "6,9",
                    "value": 69
                },
                {
                    "name": "7",
                    "value": 70
                },
                {
                    "name": "7,1",
                    "value": 71
                },
                {
                    "name": "7,2",
                    "value": 72
                },
                {
                    "name": "7,3",
                    "value": 73
                },
                {
                    "name": "7,4",
                    "value": 74
                },
                {
                    "name": "7,5",
                    "value": 75
                },
                {
                    "name": "7,6",
                    "value": 76
                },
                {
                    "name": "7,7",
                    "value": 77
                },
                {
                    "name": "7,8",
                    "value": 78
                },
                {
                    "name": "7,9",
                    "value": 79
                },
                {
                    "name": "8",
                    "value": 80
                },
                {
                    "name": "8,1",
                    "value": 81
                },
                {
                    "name": "8,2",
                    "value": 82
                },
                {
                    "name": "8,3",
                    "value": 83
                },
                {
                    "name": "8,4",
                    "value": 84
                },
                {
                    "name": "8,5",
                    "value": 85
                },
                {
                    "name": "8,6",
                    "value": 86
                },
                {
                    "name": "8,7",
                    "value": 87
                },
                {
                    "name": "8,8",
                    "value": 88
                },
                {
                    "name": "8,9",
                    "value": 89
                },
                {
                    "name": "9",
                    "value": 90
                },
                {
                    "name": "9,1",
                    "value": 91
                },
                {
                    "name": "9,2",
                    "value": 92
                },
                {
                    "name": "9,3",
                    "value": 93
                },
                {
                    "name": "9,4",
                    "value": 94
                },
                {
                    "name": "9,5",
                    "value": 95
                },
                {
                    "name": "9,6",
                    "value": 96
                },
                {
                    "name": "9,7",
                    "value": 97
                },
                {
                    "name": "9,8",
                    "value": 98
                },
                {
                    "name": "9,9",
                    "value": 99
                },
                {
                    "name": "10",
                    "value": 100
                },
                {
                    "name": "10,1",
                    "value": 101
                },
                {
                    "name": "10,2",
                    "value": 102
                },
                {
                    "name": "10,3",
                    "value": 103
                },
                {
                    "name": "10,4",
                    "value": 104
                },
                {
                    "name": "10,5",
                    "value": 105
                },
                {
                    "name": "10,6",
                    "value": 106
                },
                {
                    "name": "10,7",
                    "value": 107
                },
                {
                    "name": "10,8",
                    "value": 108
                },
                {
                    "name": "10,9",
                    "value": 109
                },
                {
                    "name": "11",
                    "value": 110
                },
                {
                    "name": "11,1",
                    "value": 111
                },
                {
                    "name": "11,2",
                    "value": 112
                },
                {
                    "name": "11,3",
                    "value": 113
                },
                {
                    "name": "11,4",
                    "value": 114
                },
                {
                    "name": "11,5",
                    "value": 115
                },
                {
                    "name": "11,6",
                    "value": 116
                },
                {
                    "name": "11,7",
                    "value": 117
                },
                {
                    "name": "11,8",
                    "value": 118
                },
                {
                    "name": "11,9",
                    "value": 119
                },
                {
                    "name": "12",
                    "value": 120
                },
                {
                    "name": "12,1",
                    "value": 121
                },
                {
                    "name": "12,2",
                    "value": 122
                },
                {
                    "name": "12,3",
                    "value": 123
                },
                {
                    "name": "12,4",
                    "value": 124
                },
                {
                    "name": "12,5",
                    "value": 125
                },
                {
                    "name": "12,6",
                    "value": 126
                },
                {
                    "name": "12,7",
                    "value": 127
                },
                {
                    "name": "12,8",
                    "value": 128
                },
                {
                    "name": "12,9",
                    "value": 129
                },
                {
                    "name": "13",
                    "value": 130
                },
                {
                    "name": "13,1",
                    "value": 131
                },
                {
                    "name": "13,2",
                    "value": 132
                },
                {
                    "name": "13,3",
                    "value": 133
                },
                {
                    "name": "13,4",
                    "value": 134
                },
                {
                    "name": "13,5",
                    "value": 135
                },
                {
                    "name": "13,6",
                    "value": 136
                },
                {
                    "name": "13,7",
                    "value": 137
                },
                {
                    "name": "13,8",
                    "value": 138
                },
                {
                    "name": "13,9",
                    "value": 139
                },
                {
                    "name": "14",
                    "value": 140
                },
                {
                    "name": "14,1",
                    "value": 141
                },
                {
                    "name": "14,2",
                    "value": 142
                },
                {
                    "name": "14,3",
                    "value": 143
                },
                {
                    "name": "14,4",
                    "value": 144
                },
                {
                    "name": "14,5",
                    "value": 145
                },
                {
                    "name": "14,6",
                    "value": 146
                },
                {
                    "name": "14,7",
                    "value": 147
                },
                {
                    "name": "14,8",
                    "value": 148
                },
                {
                    "name": "14,9",
                    "value": 149
                },
                {
                    "name": "15",
                    "value": 150
                }
            ],
            "addDescPostfix": "V",
            "addDescPrefix": "voltage",
            "addDescUseDesc": 1,
            "bgColor": "#ffd500",
            "code": 165,
            "desc": "Ionistors overcharg. (more than 8.5 V)"
        },
        {
            "addDesc": 0,
            "addDescUseDesc": 0,
            "bgColor": "#ffd500",
            "code": 170,
            "desc": "FSD IR LED fault"
        },
        {
            "addDesc": 1,
            "addDescPostfix": "un.",
            "addDescPrefix": "dustiness",
            "addDescUseDesc": 0,
            "bgColor": "#7fff00",
            "code": 171,
            "desc": "FSD initialization completed"
        },
        {
            "addDesc": 1,
            "addDescDesc": [
                {
                    "name": "ionistors voltage 0 V",
                    "value": 1
                },
                {
                    "name": "10 no answers",
                    "value": 2
                }
            ],
            "addDescUseDesc": 1,
            "bgColor": "#fff9c3",
            "code": 179,
            "desc": "Internal error"
        },
        {
            "addDesc": 1,
            "addDescDesc": [
                {
                    "name": "set to 55 °C",
                    "value": 0
                }
            ],
            "addDescUseDesc": 1,
            "bgColor": "#fff9c3",
            "code": 180,
            "desc": "No threshold temperature"
        },
        {
            "addDesc": 1,
            "addDescPrefix": "address",
            "addDescUseDesc": 0,
            "bgColor": "#ffb4b4",
            "code": 181,
            "desc": "Activate sprinkler comm. is in buffer"
        },
        {
            "addDesc": 1,
            "addDescPrefix": "address",
            "addDescUseDesc": 0,
            "bgColor": "#fff9c3",
            "code": 182,
            "desc": "Activate sprinkler comm. NOT in buffer"
        },
        {
            "addDesc": 1,
            "addDescDesc": [
                {
                    "name": "Request ionitors voltage",
                    "value": 2
                },
                {
                    "name": "Request sprinkler resistance",
                    "value": 3
                },
                {
                    "name": "Request U of lower ionistor",
                    "value": 5
                },
                {
                    "name": "Request U of middle ionistor",
                    "value": 6
                },
                {
                    "name": "Request U of upper ionistor",
                    "value": 7
                },
                {
                    "name": "Request main power supply U (_MC_)",
                    "value": 16
                },
                {
                    "name": "Request backup power supply U (_MC_)",
                    "value": 17
                },
                {
                    "name": "Request drive power supply U (_MC_)",
                    "value": 18
                },
                {
                    "name": "Request W1 Limit (FFD)",
                    "value": 19
                },
                {
                    "name": "Request W2 Limit (FFD)",
                    "value": 20
                },
                {
                    "name": "Request W3 Limit (FFD)",
                    "value": 21
                },
                {
                    "name": "Request MCU2 type and FW version",
                    "value": 22
                },
                {
                    "name": "Check FFD pyrosensor",
                    "value": 63
                },
                {
                    "name": "Ionistors charge ON",
                    "value": 64
                },
                {
                    "name": "Ionistors charge OFF",
                    "value": 65
                },
                {
                    "name": "EAS (sprinkler) heating ON",
                    "value": 66
                },
                {
                    "name": "EAS (sprinkler) heating OFF",
                    "value": 67
                },
                {
                    "name": "Red LED ON",
                    "value": 68
                },
                {
                    "name": "Red LED OFF",
                    "value": 69
                },
                {
                    "name": "Yellow LED ON",
                    "value": 70
                },
                {
                    "name": "Yellow LED OFF",
                    "value": 71
                },
                {
                    "name": "\"Test\" mode ON",
                    "value": 72
                },
                {
                    "name": "\"Test\" mode OFF",
                    "value": 73
                },
                {
                    "name": "CLOSE left isolator",
                    "value": 74
                },
                {
                    "name": "OPEN left isolator",
                    "value": 75
                },
                {
                    "name": "CLOSE right isolator",
                    "value": 76
                },
                {
                    "name": "OPEN right isolator",
                    "value": 77
                },
                {
                    "name": "Laser ON (FFD)",
                    "value": 78
                },
                {
                    "name": "Laser OFF (FFD)",
                    "value": 79
                },
                {
                    "name": "CLOSE relay 1 (RMM)",
                    "value": 81
                },
                {
                    "name": "CLOSE relay 2 (RMM)",
                    "value": 82
                },
                {
                    "name": "CLOSE relays 1, 2 (RMM)",
                    "value": 83
                },
                {
                    "name": "CLOSE relay 3 (RMM)",
                    "value": 84
                },
                {
                    "name": "CLOSE relays 1, 3 (RMM)",
                    "value": 85
                },
                {
                    "name": "CLOSE relays 2, 3 (RMM)",
                    "value": 86
                },
                {
                    "name": "CLOSE relays 1-3 (RMM)",
                    "value": 87
                },
                {
                    "name": "CLOSE relay 4 (RMM)",
                    "value": 88
                },
                {
                    "name": "CLOSE relays 1, 4 (RMM)",
                    "value": 89
                },
                {
                    "name": "CLOSE relays 2, 4 (RMM)",
                    "value": 90
                },
                {
                    "name": "CLOSE relays 1, 2, 4 (RMM)",
                    "value": 91
                },
                {
                    "name": "CLOSE relays 3, 4 (RMM)",
                    "value": 92
                },
                {
                    "name": "CLOSE relays 1, 3, 4 (RMM)",
                    "value": 93
                },
                {
                    "name": "CLOSE relays 2-4 (RMM)",
                    "value": 94
                },
                {
                    "name": "CLOSE relays 1-4 (RMM)",
                    "value": 95
                },
                {
                    "name": "ALC (AMM) in direct polarity mode",
                    "value": 96
                },
                {
                    "name": "ALC (AMM) in direct mode + flashing",
                    "value": 97
                },
                {
                    "name": "ALC (AMM) in reverse polarity mode",
                    "value": 98
                },
                {
                    "name": "ALC (AMM) in reverse mode + flashing",
                    "value": 99
                },
                {
                    "name": "OFF all relay (_MC_)",
                    "value": 106
                },
                {
                    "name": "ON relay K1 (_MC_)",
                    "value": 107
                },
                {
                    "name": "ON relay K2 (_MC_)",
                    "value": 108
                },
                {
                    "name": "OPEN relay 1 (RMM)",
                    "value": 113
                },
                {
                    "name": "OPEN relay 2 (RMM)",
                    "value": 114
                },
                {
                    "name": "OPEN relays 1, 2 (RMM)",
                    "value": 115
                },
                {
                    "name": "OPEN relay 3 (RMM)",
                    "value": 116
                },
                {
                    "name": "OPEN relays 1, 3 (RMM)",
                    "value": 117
                },
                {
                    "name": "OPEN relays 2, 3 (RMM)",
                    "value": 118
                },
                {
                    "name": "OPEN relays 1-3 (RMM)",
                    "value": 119
                },
                {
                    "name": "OPEN relay 4 (RMM)",
                    "value": 120
                },
                {
                    "name": "OPEN relays 1, 4 (RMM)",
                    "value": 121
                },
                {
                    "name": "OPEN relays 2, 4 (RMM)",
                    "value": 122
                },
                {
                    "name": "OPEN relays 1, 2, 4 (RMM)",
                    "value": 123
                },
                {
                    "name": "OPEN relays 3, 4 (RMM)",
                    "value": 124
                },
                {
                    "name": "OPEN relays 1, 3, 4 (RMM)",
                    "value": 125
                },
                {
                    "name": "OPEN relays 2-4 (RMM)",
                    "value": 126
                },
                {
                    "name": "OPEN relays 1-4 (RMM)",
                    "value": 127
                },
                {
                    "name": "Change AD address",
                    "value": 128
                },
                {
                    "name": "Record W1 Limit (FFD)",
                    "value": 140
                },
                {
                    "name": "Record W2 Limit (FFD)",
                    "value": 141
                },
                {
                    "name": "Record W3 Limit (FFD)",
                    "value": 142
                }
            ],
            "addDescUseDesc": 1,
            "bgColor": "#fff9c3",
            "code": 183,
            "desc": "Command failed (wrong AD type)"
        },
        {
            "addDesc": 1,
            "addDescDesc": [
                {
                    "name": "EAS (sprinkler) heating ON",
                    "value": 66
                },
                {
                    "name": "EAS (sprinkler) heating OFF",
                    "value": 67
                },
                {
                    "name": "\"Test\" mode ON",
                    "value": 72
                },
                {
                    "name": "\"Test\" mode OFF",
                    "value": 73
                },
                {
                    "name": "Laser ON (FFD)",
                    "value": 78
                },
                {
                    "name": "Laser OFF (FFD)",
                    "value": 79
                }
            ],
            "addDescUseDesc": 1,
            "bgColor": "#fff9c3",
            "code": 184,
            "desc": "Command failed (ionistors discharged)"
        },
        {
            "addDesc": 1,
            "addDescDesc": [
                {
                    "name": "EAS (sprinkler) heating ON",
                    "value": 66
                },
                {
                    "name": "EAS (sprinkler) heating OFF",
                    "value": 67
                },
                {
                    "name": "Laser ON (FFD)",
                    "value": 78
                },
                {
                    "name": "Laser OFF (FFD)",
                    "value": 79
                }
            ],
            "addDescUseDesc": 1,
            "bgColor": "#fff9c3",
            "code": 185,
            "desc": "Command failed (sprinkler fault)"
        },
        {
            "addDesc": 1,
            "addDescDesc": [
                {
                    "name": "Request AD type",
                    "value": 1
                },
                {
                    "name": "Request ionitors voltage",
                    "value": 2
                },
                {
                    "name": "Request sprinkler resistance",
                    "value": 3
                },
                {
                    "name": "Request U of lower ionistor",
                    "value": 5
                },
                {
                    "name": "Request U of middle ionistor",
                    "value": 6
                },
                {
                    "name": "Request U of upper ionistor",
                    "value": 7
                },
                {
                    "name": "Request processor type",
                    "value": 15
                },
                {
                    "name": "Request main power supply U (_MC_)",
                    "value": 16
                },
                {
                    "name": "Request backup power supply U (_MC_)",
                    "value": 17
                },
                {
                    "name": "Request drive power supply U (_MC_)",
                    "value": 18
                },
                {
                    "name": "Request W1 Limit (FFD)",
                    "value": 19
                },
                {
                    "name": "Request W2 Limit (FFD)",
                    "value": 20
                },
                {
                    "name": "Request W3 Limit (FFD)",
                    "value": 21
                },
                {
                    "name": "Request MCU2 type and FW version",
                    "value": 22
                },
                {
                    "name": "Check FFD pyrosensor",
                    "value": 63
                },
                {
                    "name": "Ionistors charge ON",
                    "value": 64
                },
                {
                    "name": "Ionistors charge OFF",
                    "value": 65
                },
                {
                    "name": "EAS (sprinkler) heating ON",
                    "value": 66
                },
                {
                    "name": "EAS (sprinkler) heating OFF",
                    "value": 67
                },
                {
                    "name": "Red LED ON",
                    "value": 68
                },
                {
                    "name": "Red LED OFF",
                    "value": 69
                },
                {
                    "name": "Yellow LED ON",
                    "value": 70
                },
                {
                    "name": "Yellow LED OFF",
                    "value": 71
                },
                {
                    "name": "\"Test\" mode ON",
                    "value": 72
                },
                {
                    "name": "\"Test\" mode OFF",
                    "value": 73
                },
                {
                    "name": "CLOSE left isolator",
                    "value": 74
                },
                {
                    "name": "OPEN left isolator",
                    "value": 75
                },
                {
                    "name": "CLOSE right isolator",
                    "value": 76
                },
                {
                    "name": "OPEN right isolator",
                    "value": 77
                },
                {
                    "name": "Laser ON (FFD)",
                    "value": 78
                },
                {
                    "name": "Laser OFF (FFD)",
                    "value": 79
                },
                {
                    "name": "CLOSE relay 1 (RMM)",
                    "value": 81
                },
                {
                    "name": "CLOSE relay 2 (RMM)",
                    "value": 82
                },
                {
                    "name": "CLOSE relays 1, 2 (RMM)",
                    "value": 83
                },
                {
                    "name": "CLOSE relay 3 (RMM)",
                    "value": 84
                },
                {
                    "name": "CLOSE relays 1, 3 (RMM)",
                    "value": 85
                },
                {
                    "name": "CLOSE relays 2, 3 (RMM)",
                    "value": 86
                },
                {
                    "name": "CLOSE relays 1-3 (RMM)",
                    "value": 87
                },
                {
                    "name": "CLOSE relay 4 (RMM)",
                    "value": 88
                },
                {
                    "name": "CLOSE relays 1, 4 (RMM)",
                    "value": 89
                },
                {
                    "name": "CLOSE relays 2, 4 (RMM)",
                    "value": 90
                },
                {
                    "name": "CLOSE relays 1, 2, 4 (RMM)",
                    "value": 91
                },
                {
                    "name": "CLOSE relays 3, 4 (RMM)",
                    "value": 92
                },
                {
                    "name": "CLOSE relays 1, 3, 4 (RMM)",
                    "value": 93
                },
                {
                    "name": "CLOSE relays 2-4 (RMM)",
                    "value": 94
                },
                {
                    "name": "CLOSE relays 1-4 (RMM)",
                    "value": 95
                },
                {
                    "name": "ALC (AMM) in direct polarity mode",
                    "value": 96
                },
                {
                    "name": "ALC (AMM) in direct mode + flashing",
                    "value": 97
                },
                {
                    "name": "ALC (AMM) in reverse polarity mode",
                    "value": 98
                },
                {
                    "name": "ALC (AMM) in reverse mode + flashing",
                    "value": 99
                },
                {
                    "name": "Discharge resistor ON",
                    "value": 100
                },
                {
                    "name": "Discharge resistor OFF",
                    "value": 101
                },
                {
                    "name": "Photopath test",
                    "value": 102
                },
                {
                    "name": "OFF all relay (_MC_)",
                    "value": 106
                },
                {
                    "name": "ON relay K1 (_MC_)",
                    "value": 107
                },
                {
                    "name": "ON relay K2 (_MC_)",
                    "value": 108
                },
                {
                    "name": "OPEN relay (RMM)",
                    "value": 112
                },
                {
                    "name": "OPEN relay 1 (RMM)",
                    "value": 113
                },
                {
                    "name": "OPEN relay 2 (RMM)",
                    "value": 114
                },
                {
                    "name": "OPEN relays 1, 2 (RMM)",
                    "value": 115
                },
                {
                    "name": "OPEN relay 3 (RMM)",
                    "value": 116
                },
                {
                    "name": "OPEN relays 1, 3 (RMM)",
                    "value": 117
                },
                {
                    "name": "OPEN relays 2, 3 (RMM)",
                    "value": 118
                },
                {
                    "name": "OPEN relays 1-3 (RMM)",
                    "value": 119
                },
                {
                    "name": "OPEN relay 4 (RMM)",
                    "value": 120
                },
                {
                    "name": "OPEN relays 1, 4 (RMM)",
                    "value": 121
                },
                {
                    "name": "OPEN relays 2, 4 (RMM)",
                    "value": 122
                },
                {
                    "name": "OPEN relays 1, 2, 4 (RMM)",
                    "value": 123
                },
                {
                    "name": "OPEN relays 3, 4 (RMM)",
                    "value": 124
                },
                {
                    "name": "OPEN relays 1, 3, 4 (RMM)",
                    "value": 125
                },
                {
                    "name": "OPEN relays 2-4 (RMM)",
                    "value": 126
                },
                {
                    "name": "OPEN relays 1-4 (RMM)",
                    "value": 127
                },
                {
                    "name": "Change AD address",
                    "value": 128
                },
                {
                    "name": "Record W1 Limit (FFD)",
                    "value": 140
                },
                {
                    "name": "Record W2 Limit (FFD)",
                    "value": 141
                },
                {
                    "name": "Record W3 Limit (FFD)",
                    "value": 142
                }
            ],
            "addDescUseDesc": 1,
            "bgColor": "#fff9c3",
            "code": 186,
            "desc": "Command failed (no conn. / disabl. AD)"
        },
        {
            "addDesc": 1,
            "addDescDesc": [
                {
                    "name": "Check FFD pyrosensor",
                    "value": 63
                },
                {
                    "name": "Ionistors charge ON",
                    "value": 64
                },
                {
                    "name": "Ionistors charge OFF",
                    "value": 65
                },
                {
                    "name": "EAS (sprinkler) heating ON",
                    "value": 66
                },
                {
                    "name": "EAS (sprinkler) heating OFF",
                    "value": 67
                },
                {
                    "name": "\"Test\" mode ON",
                    "value": 72
                },
                {
                    "name": "\"Test\" mode OFF",
                    "value": 73
                },
                {
                    "name": "Laser ON (FFD)",
                    "value": 78
                },
                {
                    "name": "Laser OFF (FFD)",
                    "value": 79
                }
            ],
            "addDescUseDesc": 1,
            "bgColor": "#fff9c3",
            "code": 187,
            "desc": "Command failed (sprinkler is open)"
        },
        {
            "addDesc": 1,
            "addDescDesc": [
                {
                    "name": "Check FFD pyrosensor",
                    "value": 63
                },
                {
                    "name": "Ionistors charge ON",
                    "value": 64
                },
                {
                    "name": "Ionistors charge OFF",
                    "value": 65
                },
                {
                    "name": "EAS (sprinkler) heating ON",
                    "value": 66
                },
                {
                    "name": "EAS (sprinkler) heating OFF",
                    "value": 67
                },
                {
                    "name": "\"Test\" mode ON",
                    "value": 72
                },
                {
                    "name": "\"Test\" mode OFF",
                    "value": 73
                },
                {
                    "name": "Laser ON (FFD)",
                    "value": 78
                },
                {
                    "name": "Laser OFF (FFD)",
                    "value": 79
                },
                {
                    "name": "Change AD address",
                    "value": 128
                }
            ],
            "addDescUseDesc": 1,
            "bgColor": "#fff9c3",
            "code": 188,
            "desc": "Command failed (ionistors fault)"
        },
        {
            "addDesc": 0,
            "addDescUseDesc": 0,
            "bgColor": "#ffd500",
            "code": 189,
            "desc": "Heating complete, sprinkler NOT opened"
        },
        {
            "addDesc": 1,
            "addDescDesc": [
                {
                    "name": "after activation",
                    "value": 1
                },
                {
                    "name": "after fault",
                    "value": 2
                },
                {
                    "name": "after opening",
                    "value": 5
                },
                {
                    "name": "after was shorted",
                    "value": 6
                }
            ],
            "addDescUseDesc": 1,
            "bgColor": "#7fff00",
            "code": 190,
            "desc": "Sprinkler is Ok",
            "fgColor": "#000000"
        },
        {
            "addDesc": 1,
            "addDescDesc": [
                {
                    "name": "after fault",
                    "value": 0
                }
            ],
            "addDescUseDesc": 1,
            "bgColor": "#7fff00",
            "code": 191,
            "desc": "Temperature sensor is Ok"
        },
        {
            "addDesc": 1,
            "addDescDesc": [
                {
                    "name": "after fault",
                    "value": 0
                }
            ],
            "addDescUseDesc": 1,
            "bgColor": "#7fff00",
            "code": 192,
            "desc": "IR LED (FSD) is Ok"
        },
        {
            "addDesc": 1,
            "addDescPostfix": "°C",
            "addDescPrefix": "t=",
            "addDescUseDesc": 0,
            "bgColor": "#ffb4b4",
            "code": 193,
            "desc": "Pre-alarm (80% of temper. threshold)"
        },
        {
            "addDesc": 0,
            "addDescUseDesc": 0,
            "code": 194,
            "desc": "IMM input contact is open"
        },
        {
            "addDesc": 1,
            "addDescDesc": [
                {
                    "name": "MCP",
                    "value": 1
                },
                {
                    "name": "FHD",
                    "value": 2
                },
                {
                    "name": "FHD-S",
                    "value": 3
                },
                {
                    "name": "FSD",
                    "value": 4
                },
                {
                    "name": "FFD",
                    "value": 5
                },
                {
                    "name": "FFD-S",
                    "value": 6
                },
                {
                    "name": "RAU",
                    "value": 7
                },
                {
                    "name": "IMM2",
                    "value": 8
                },
                {
                    "name": "IMM4",
                    "value": 9
                },
                {
                    "name": "RMM2",
                    "value": 10
                },
                {
                    "name": "RMM4",
                    "value": 11
                },
                {
                    "name": "MCP-B",
                    "value": 12
                },
                {
                    "name": "IRMM22",
                    "value": 13
                },
                {
                    "name": "IMM2A",
                    "value": 14
                },
                {
                    "name": "AMM(E)",
                    "value": 15
                },
                {
                    "name": "AMM(S)",
                    "value": 16
                },
                {
                    "name": "SMM",
                    "value": 17
                },
                {
                    "name": "_MC_",
                    "value": 18
                },
                {
                    "name": "_MCB_",
                    "value": 19
                },
                {
                    "name": "_MCBP_",
                    "value": 20
                },
                {
                    "name": "_MCR_",
                    "value": 21
                },
                {
                    "name": "_MCRS_",
                    "value": 22
                },
                {
                    "name": "FS/HD",
                    "value": 23
                },
                {
                    "name": "FS/HD-S",
                    "value": 24
                }
            ],
            "addDescUseDesc": 1,
            "code": 195,
            "desc": "FW preamble transferred successfully"
        },
        {
            "addDesc": 1,
            "addDescPostfix": "un.",
            "addDescUseDesc": 0,
            "bgColor": "#ffd500",
            "code": 196,
            "desc": "FSD photopath fault"
        },
        {
            "addDesc": 1,
            "addDescPostfix": "un.",
            "addDescUseDesc": 0,
            "bgColor": "#7fff00",
            "code": 197,
            "desc": "FSD photopath is Ok (after fault)"
        },
        {
            "addDesc": 1,
            "addDescPostfix": "un.",
            "addDescPrefix": "dustiness",
            "addDescUseDesc": 0,
            "bgColor": "#fff9c3",
            "code": 198,
            "desc": "Critical FSD dustiness (maint. req.)"
        },
        {
            "addDesc": 1,
            "addDescPostfix": "un.",
            "addDescPrefix": "dustiness",
            "addDescUseDesc": 0,
            "bgColor": "Gold",
            "code": 199,
            "desc": "Maximum FSD dustiness"
        },
        {
            "addDesc": 1,
            "addDescPostfix": "un.",
            "addDescPrefix": "current ADC value",
            "addDescUseDesc": 0,
            "bgColor": "#7fff00",
            "code": 200,
            "desc": "FSD initializ. (smoke chamber cleared)"
        },
        {
            "addDesc": 0,
            "addDescUseDesc": 0,
            "bgColor": "#ffd500",
            "code": 201,
            "desc": "Valve is in middle position"
        },
        {
            "addDesc": 0,
            "addDescUseDesc": 0,
            "code": 202,
            "desc": "Valve is open"
        },
        {
            "addDesc": 0,
            "addDescUseDesc": 0,
            "code": 203,
            "desc": "Valve is closed"
        },
        {
            "addDesc": 0,
            "addDescUseDesc": 0,
            "bgColor": "#ffd500",
            "code": 204,
            "desc": "Fault of valve control circuit"
        },
        {
            "addDesc": 0,
            "addDescUseDesc": 0,
            "bgColor": "#ffd500",
            "code": 205,
            "desc": "ALC is open"
        },
        {
            "addDesc": 0,
            "addDescUseDesc": 0,
            "bgColor": "#ffd500",
            "code": 206,
            "desc": "ALC is shorted"
        },
        {
            "addDesc": 1,
            "addDescDesc": [
                {
                    "name": "ALC powered",
                    "value": 0
                },
                {
                    "name": "after ALC was shorted",
                    "value": 1
                },
                {
                    "name": "after ALC opening",
                    "value": 2
                }
            ],
            "addDescUseDesc": 1,
            "bgColor": "#7fff00",
            "code": 207,
            "desc": "ALC is Ok"
        },
        {
            "addDesc": 0,
            "addDescUseDesc": 0,
            "bgColor": "#ffd500",
            "code": 208,
            "desc": "No power in ALC"
        },
        {
            "addDesc": 0,
            "addDescUseDesc": 0,
            "code": 209,
            "desc": "ALC - direct polarity with flashing"
        },
        {
            "addDesc": 0,
            "addDescUseDesc": 0,
            "code": 210,
            "desc": "ALC - reverse polarity with flashing"
        },
        {
            "addDesc": 0,
            "addDescUseDesc": 0,
            "code": 211,
            "desc": "ALC - reverse polarity"
        },
        {
            "addDesc": 0,
            "addDescUseDesc": 0,
            "code": 212,
            "desc": "ALC - direct polarity"
        },
        {
            "addDesc": 0,
            "addDescUseDesc": 0,
            "bgColor": "#7fff00",
            "code": 214,
            "desc": "Device firmware successfully updated"
        },
        {
            "addDesc": 1,
            "addDescDesc": [
                {
                    "name": "FW type error",
                    "value": 1
                },
                {
                    "name": "packet CRC error",
                    "value": 2
                },
                {
                    "name": "packet transmission sequence error",
                    "value": 3
                },
                {
                    "name": "AD memory shortage",
                    "value": 4
                },
                {
                    "name": "FW integrity bit = 0",
                    "value": 5
                },
                {
                    "name": "FW size error",
                    "value": 6
                }
            ],
            "addDescUseDesc": 1,
            "bgColor": "#fff9c3",
            "code": 215,
            "desc": "FW transfer interrupted"
        },
        {
            "addDesc": 0,
            "addDescUseDesc": 0,
            "code": 216,
            "desc": "Preamble transferred, FW transfer"
        },
        {
            "addDesc": 0,
            "addDescUseDesc": 0,
            "code": 217,
            "desc": "FW transferred, CRC check"
        },
        {
            "addDesc": 1,
            "addDescDesc": [
                {
                    "name": "packet num. equal to alr. transmitted",
                    "value": 1
                },
                {
                    "name": "command not accep. or AD not respon.",
                    "value": 2
                },
                {
                    "name": "trans. and req. packets are different",
                    "value": 3
                }
            ],
            "addDescUseDesc": 1,
            "bgColor": "#fff9c3",
            "code": 218,
            "desc": "Retransmission of FW package"
        },
        {
            "addDesc": 0,
            "addDescUseDesc": 0,
            "bgColor": "#fff9c3",
            "code": 219,
            "desc": "Firmware CRC error"
        },
        {
            "addDesc": 1,
            "addDescDesc": [
                {
                    "name": "MCP",
                    "value": 1
                },
                {
                    "name": "FHD",
                    "value": 2
                },
                {
                    "name": "FHD-S",
                    "value": 3
                },
                {
                    "name": "FSD",
                    "value": 4
                },
                {
                    "name": "FFD",
                    "value": 5
                },
                {
                    "name": "FFD-S",
                    "value": 6
                },
                {
                    "name": "RAU",
                    "value": 7
                },
                {
                    "name": "IMM2",
                    "value": 8
                },
                {
                    "name": "IMM4",
                    "value": 9
                },
                {
                    "name": "RMM2",
                    "value": 10
                },
                {
                    "name": "RMM4",
                    "value": 11
                },
                {
                    "name": "MCP-B",
                    "value": 12
                },
                {
                    "name": "IRMM22",
                    "value": 13
                },
                {
                    "name": "IMM2A",
                    "value": 14
                },
                {
                    "name": "AMM(E)",
                    "value": 15
                },
                {
                    "name": "AMM(S)",
                    "value": 16
                },
                {
                    "name": "SMM",
                    "value": 17
                },
                {
                    "name": "_MC_",
                    "value": 18
                },
                {
                    "name": "_MCB_",
                    "value": 19
                },
                {
                    "name": "_MCBP_",
                    "value": 20
                },
                {
                    "name": "_MCR_",
                    "value": 21
                },
                {
                    "name": "_MCRS_",
                    "value": 22
                },
                {
                    "name": "FS/HD",
                    "value": 23
                },
                {
                    "name": "FS/HD-S",
                    "value": 24
                }
            ],
            "addDescUseDesc": 1,
            "code": 220,
            "desc": "FW delivered successfully (to LC)"
        },
        {
            "addDesc": 0,
            "addDescUseDesc": 0,
            "bgColor": "#ffffff",
            "code": 221,
            "desc": "Laser is off"
        },
        {
            "addDesc": 0,
            "addDescUseDesc": 0,
            "code": 222,
            "desc": "Laser is on"
        },
        {
            "addDesc": 1,
            "addDescDesc": [
                {
                    "name": "pyroprocessor",
                    "value": 2
                },
                {
                    "name": "pyrosensor or amplifier",
                    "value": 3
                }
            ],
            "addDescUseDesc": 1,
            "bgColor": "#ffd500",
            "code": 223,
            "desc": "Pyrospath fault (FFD)"
        },
        {
            "addDesc": 1,
            "addDescDesc": [
                {
                    "name": "after a pyrosensor fault",
                    "value": 2
                },
                {
                    "name": "after a pyrosensor or amplifier fault",
                    "value": 3
                }
            ],
            "addDescUseDesc": 1,
            "bgColor": "#7fff00",
            "code": 224,
            "desc": "Pyrospath is Ok (FFD)"
        },
        {
            "addDesc": 1,
            "addDescUseDesc": 0,
            "code": 225,
            "desc": "Pyrosensor check (FFD)"
        },
        {
            "addDesc": 0,
            "addDescUseDesc": 0,
            "bgColor": "#ffd500",
            "code": 226,
            "desc": "Engine power supply fault"
        },
        {
            "addDesc": 0,
            "addDescUseDesc": 0,
            "bgColor": "#7fff00",
            "code": 227,
            "desc": "Engine power supply is Ok"
        },
        {
            "addDesc": 1,
            "addDescDesc": [
                {
                    "name": "MCP",
                    "value": 1
                },
                {
                    "name": "FHD",
                    "value": 2
                },
                {
                    "name": "FHD-S",
                    "value": 3
                },
                {
                    "name": "FSD",
                    "value": 4
                },
                {
                    "name": "FFD",
                    "value": 5
                },
                {
                    "name": "FFD-S",
                    "value": 6
                },
                {
                    "name": "RAU",
                    "value": 7
                },
                {
                    "name": "IMM2",
                    "value": 8
                },
                {
                    "name": "IMM4",
                    "value": 9
                },
                {
                    "name": "RMM2",
                    "value": 10
                },
                {
                    "name": "RMM4",
                    "value": 11
                },
                {
                    "name": "MCP-B",
                    "value": 12
                },
                {
                    "name": "IRMM22",
                    "value": 13
                },
                {
                    "name": "IMM2A",
                    "value": 14
                },
                {
                    "name": "AMM(E)",
                    "value": 15
                },
                {
                    "name": "AMM(S)",
                    "value": 16
                },
                {
                    "name": "SMM",
                    "value": 17
                },
                {
                    "name": "_MC_",
                    "value": 18
                },
                {
                    "name": "_MCB_",
                    "value": 19
                },
                {
                    "name": "_MCBP_",
                    "value": 20
                },
                {
                    "name": "_MCR_",
                    "value": 21
                },
                {
                    "name": "_MCRS_",
                    "value": 22
                },
                {
                    "name": "FS/HD",
                    "value": 23
                },
                {
                    "name": "FS/HD-S",
                    "value": 24
                }
            ],
            "addDescUseDesc": 1,
            "bgColor": "#fff9c3",
            "code": 228,
            "desc": "FW size error"
        }
    ],
    "lang": "RU",
    "version": 2
}
