{
	"content": "Gefest TestKl events description",
	"version": 1,
	"lang": "RU",
	"data": [
		{
			"code": 1,
			"bgColor": "Aqua",
			"desc": "error: cannot create an OS kernel object (task, queue, semaphore or mutex)"
		},
		{
			"code": 2,
			"bgColor": "Aqua",
			"desc": "error: message lost due to overflow of message queue sent from tasks"
		},
		{
			"code": 3,
			"bgColor": "Aqua",
			"desc": "error: message lost due to message queue overflow from interrupts"
		},
		{
			"code": 4,
			"bgColor": "Aqua",
			"desc": "error: the semaphore in the task_InitLS function was not released during the initialization process - 120 µS"
		},
		{
			"code": 5,
			"bgColor": "Aqua",
			"desc": "error: the semaphore in the task_InitLS function was not released during the initialization of the right direction - 20 ms"
		},
		{
			"code": 6,
			"bgColor": "Aqua",
			"desc": "error: the semaphore in the task_InitLS function was not released during the initialization process - 0.7 ms"
		},
		{
			"code": 7,
			"bgColor": "Aqua",
			"desc": "error: the semaphore in the task_InitLS function was not released during the initialization process - 120 µS"
		},
		{
			"code": 8,
			"bgColor": "Aqua",
			"desc": "error: the semaphore in the task_InitLS function was not released during the initialization process - 20 ms"
		},
		{
			"code": 9,
			"bgColor": "Aqua",
			"desc": "error: the semaphore in the task_InitLS function was not released during the initialization process - 75 C"
		},
		{
			"code": 10,
			"bgColor": "Aqua",
			"desc": "error: the semaphore in the task_InitLS function was not released during the initialization of the left direction - 20 ms"
		},
		{
			"code": 11,
			"bgColor": "Aqua",
			"desc": "error: the semaphore in the task_InitLS function was not released during the initialization of the left direction - 75"
		},
		{
			"code": 12,
			"bgColor": "Aqua",
			"desc": "error: the semaphore in the task_InitLS function was not released during the initialization process - 120 µS when checking the right end element during the initialization process"
		},
		{
			"code": 13,
			"bgColor": "Agua",
			"desc": "error: the semaphore in the task_InitLS function was not released during the initialization process - 50 mС"
		},
		{
			"code": 14,
			"bgColor": "Aqua",
			"desc": "error: when issuing a semaphore in a function after the end of the sDelayKZ_InitRightDir or sDelayKZ_InitLeftDir interval, it was already available"
		},
		{
			"code": 15,
			"bgColor": "Aqua",
			"desc": "error: when issuing a semaphore in a function after the end of the sDelayInitLS interval, it was already available"
		},
		{
			"code": 16,
			"bgColor": "Aqua",
			"desc": "error: OS stack overflow"
		},
		{
			"code": 17,
			"bgColor": "Agua",
			"desc": "error: when issuing a semaphore in the FLASH_IRQHandler() interrupt, the semaphore was already available"
		},
		{
			"code": 18,
			"bgColor": "Agua",
			"desc": "error: failed to wait for semaphore in flash_erase_page() or flash_write() function " 
		},
		{
			"code": 19,
			"bgColor": "Aqua",
			"desc": "error: ModBus error - events were not transmitted from the CL event queue"
		},
		{
			"code": 20,
			"bgColor": "Aqua",
			"desc": "error: ModBus error - number of events not transmitted"
		},
		{
			"code": 21,
			"bgColor": "Aqua",
			"desc": "error: There was an error in the DMA channel"
		},
		{
			"code": 22,
			"bgColor": "Aqua",
			"desc": "the number of elements in the queue to which a message cannot be added due to overflow"
		},
		{
			"code": 23,
			"bgColor": "Aqua",
			"desc": "the number of free elements in the queue to which a message cannot be added due to overflow"
		},
		{
			"code": 32,
			"bgColor": "Aqua",
			"desc": "error: timer semaphore delay 75 s"
		},
		{
			"code": 33,
			"bgColor": "White",
			"desc": "error: CL initialization process was interrupted due to directly connected outputs"
		},
		{
			"code": 34,
			"bgColor": "White",
			"desc": "error: the initialization process is completed, but there is an MA with incorrectly connected polarity in the LAN"
		},
		{
			"code": 35,
			"bgColor": "White",
			"desc": "error: CL initialization process interrupted"
		},
		{
			"code": 36,
			"bgColor": "White",
			"desc": "error: The initialization process was interrupted due to an unknown error in the initialization process"
		},
		{
			"code": 39,
			"bgColor": "White",
			"desc": "AD responded to the address of the blocked device"
		},
		{
			"code": 40,
			"bgColor": "Gold",
			"desc": "for proper operation of the AD, you need to update its software"
		},
		{
			"code": 41,
			"bgColor": "White",
			"desc": "error: during the initialization of the LS, a malfunction was detected (incorrect connection of the polarity of the AD, which caused a short circuit at the right input of the KL), re-initialization of the KL is started"
		},
		{
			"code": 51,
			"bgColor": "Gold",
			"desc": "error: LS short circuit at the left input of the KL"
		},
		{
			"code": 52,
			"bgColor": "Gold",
			"desc": "error: LS short circuit at right KL input"
		},
		{
			"code": 53,
			"bgColor": "Gold",
			"desc": "error: LS interruption"
		},
		{
			"code": 54,
			"bgColor": "Gold",
			"desc": "error: SC LS"
		},
		{
			"code": 55,
			"bgColor": "Gold",
			"desc": "error: a SC LS was detected behind the device"
		},
		{
			"code": 56,
			"bgColor": "White",
			"desc": "It was not possible to detect the location of the SC"
		},
		{
			"code": 57,
			"bgColor": "White",
			"desc": "it was not possible to detect the location of the LS damage"
		},
		{
			"code": 58,
			"bgColor": "White",
			"desc": "MA data duration error (f_Err_DlitD_Small or f_Err_DlitD_Big) when receiving from AD"
		},
		{
			"code": 59,
			"bgColor": "White",
			"desc": "timeout error (f_Err_Time) when receiving data from the AD"
		},
		{
			"code": 60,
			"bgColor": "White",
			"desc": "parity bit error (f_Err_CRC) when receiving data from the AD"
		},
		{
			"code": 61,
			"bgColor": "Gold",
			"desc": "error: the maximum permissible resistance of the LS line has been exceeded, the ADs may not operate stably, the IPT ionistors cannot be charged"
		},
		{
			"code": 62,
			"bgColor": "White",
			"desc": "error: the magnitude of the response current from the MA is below the permissible threshold (35 mA for SB and 27 mA for DB)"
		},
		{
			"code": 63,
			"bgColor": "LightGreen",
			"desc": "entering, exiting or attempting to enter the Service Menu"
		},
		{
			"code": 71,
			"bgColor": "Gold",
			"desc": "error: during the initial initialization of the CL, after applying voltage to the left direction, a signal was received from the right EE"
		},
		{
			"code": 72,
			"bgColor": "White",
			"desc": "The power line has recovered after a break or short circuit (1 - Open circuit, 2 - Short circuit)"
		},
		{
			"code": 73,
			"bgColor": "White",
			"desc": "error: during the initial initialization of the CL, after applying voltage to the right direction, a signal was received from the left EE"
		},
		{
			"code": 74,
			"bgColor": "White",
			"desc": "error: left end element is faulty"
		},
		{
			"code": 75,
			"bgColor": "White",
			"desc": "error: right end element is faulty"
		},
		{
			"code": 76,
			"bgColor": "DarkOrchid",
			"desc": "error: DMA channel"
		},
		{
			"code": 77,
			"bgColor": "DarkOrchid",
			"desc": "error: for unknown reasons, bit sDEVICE.f_DriverLS_IsOn was set to 0"
		},
		{
			"code": 78,
			"bgColor": "White",
			"desc": "error: low power supply voltage"
		},
		{
			"code": 79,
			"bgColor": "White",
			"desc": "power supply voltage is normal"
		},
		{
			"code": 80,
			"bgColor": "White",
			"desc": "error: OP malfunction"
		},
		{
			"code": 81,
			"bgColor": "White",
			"desc": "error: RP malfunction"
		},
		{
			"code": 82,
			"bgColor": "White",
			"desc": "main power supply is normal"
		},
		{
			"code": 83,
			"bgColor": "White",
			"desc": "backup power is normal"
		},
		{
			"code": 85,
			"bgColor": "White",
			"desc": "error: KL case opened"
		},
		{
			"code": 86,
			"bgColor": "White",
			"desc": "KL case is closed"
		},
		{
			"code": 87,
			"bgColor": "White",
			"desc": "The configuration table was deleted successfully"
		},
		{
			"code": 88,
			"bgColor": "White",
			"desc": "Error deleting configuration table"
		},
		{
			"code": 89,
			"bgColor": "DarkOrchid",
			"desc": "for unknown reasons, the sDelayDriverLS timer has failed"
		},
		{
			"code": 90,
			"bgColor": "DarkOrchid",
			"desc": "message about the place where the safety timer was disabled"
		},
		{
			"code": 99,
			"bgColor": "DarkOrchid",
			"desc": "message about the status of the driver lock and the global control flag of the transmitter driver"
		},
		{
			"code": 100,
			"bgColor": "White",
			"desc": "a command has been entered into the command register"
		},
		{
			"code": 101,
			"bgColor": "DeepSkyBlue",
			"desc": "the KL initialization process has begun: 1 – software reset, 2 – power reset, 3 – reset by WatchDog timer, 5 – incomprehensible reset"
		},
		{
			"code": 102,
			"bgColor": "White",
			"desc": "the KL initialization process has been successfully completed"
		},
		{
			"code": 103,
			"bgColor": "White",
			"desc": "error: the LS initialization process has been completed, but there is a fault in the LS (short circuit, open circuit or device with an unprogrammed address)"
		},
		{
			"code": 104,
			"bgColor": "White",
			"desc": "the LS initialization process has been successfully completed (the LS is looped)"
		},
		{
			"code": 105,
			"bgColor": "White",
			"desc": "error: during the LS initialization process, a fault was detected in the line (short circuit, open circuit, address 251 or incorrect AD polarity connection)"
		},
		{
			"code": 106,
			"bgColor": "White",
			"desc": "left direction of the LS is connected"
		},
		{
			"code": 107,
			"bgColor": "White",
			"desc": "left direction of LS is disabled"
		},
		{
			"code": 108,
			"bgColor": "White",
			"desc": "the right direction of the LS is connected"
		},
		{
			"code": 109,
			"bgColor": "White",
			"desc": "the right direction of the LS is disabled"
		},
		{
			"code": 110,
			"bgColor": "White",
			"desc": "signal received from right KE"
		},
		{
			"code": 111,
			"bgColor": "White",
			"desc": "signal received from left KE"
		},
		{
			"code": 112,
			"bgColor": "Magenta",
			"desc": "error: device has stopped working"
		},
		{
			"code": 113,
			"bgColor": "White",
			"desc": "the process of initializing the LS on the left side has begun"
		},
		{
			"code": 114,
			"bgColor": "White",
			"desc": "the process of initializing the LS on the right side has begun"
		},
		{
			"code": 115,
			"bgColor": "Coral",
			"desc": "error: LS command buffer overflow occurred"
		},
		{
			"code": 116,
			"bgColor": "Coral",
			"desc": "error: mutex not released, command not sent"
		},
		{
			"code": 117,
			"bgColor": "DarkOrchid",
			"desc": "an error occurred while writing to FLASH"
		},
		{
			"code": 118,
			"bgColor": "White",
			"desc": "The configuration table was written successfully"
		},
		{
			"code": 120,
			"bgColor": "White",
			"desc": "error: loss of connection with AD (AD does not respond)"
		},
		{
			"code": 121,
			"bgColor": "White",
			"desc": "error: loss of connection with AD (multiple reception errors)"
		},
		{
			"code": 122,
			"bgColor": "White",
			"desc": "the previously lost connection with the AD has been restored"
		},
		{
			"code": 123,
			"bgColor": "White",
			"desc": "error: AD with unknown type detected"
		},
		{
			"code": 124,
			"bgColor": "White",
			"desc": "error: failed to issue command"
		},
		{
			"code": 125,
			"bgColor": "White",
			"desc": "error: double address detected, ionistor charging will not be turned on, and where it was previously turned on, it will be stopped"
		},
		{
			"code": 126,
			"bgColor": "White",
			"desc": "error: device with unprogrammed address 251 detected"
		},
		{
			"code": 127,
			"bgColor": "White",
			"desc": "error: device type has changed"
		},
		{
			"code": 128,
			"bgColor": "White",
			"desc": "error: device software version has changed"
		},
		{
			"code": 129,
			"bgColor": "White",
			"desc": "error: temperature sensor is faulty"
		},
		{
			"code": 130,
			"bgColor": "Coral",
			"desc": "ModBus event buffer overflow"
		},
		{
			"code": 131,
			"bgColor": "Red",
			"fgColor": "White",
			"desc": "Fire",
			"addDesc": 1,
			"addDescPrefix": "Current temperature = "
		},
		{
			"code": 133,
			"bgColor": "DarkOrchid",
			"desc": "error verifying data written to FLASH"
		},
		{
			"code": 134,
			"bgColor": "White",
			"desc": "error: ionistor is faulty (open circuit or short circuit)"
		},
		{
			"code": 135,
			"bgColor": "White",
			"desc": "The ionistor has moved from the Malfunction state (Open or short circuit) to the Normal state"
		},
		{
			"code": 136,
			"bgColor": "Gold",
			"desc": "ionistors are switched to charge mode"
		},
		{
			"code": 137,
			"bgColor": "White",
			"desc": "error: Heater malfunction (open circuit or short circuit)",
			"addDesc": 0
		},
		{
			"code": 138,
			"bgColor": "White",
			"desc": "heater is heating up",
			"addDesc": 0
		},
		{
			"code": 139,
			"bgColor": "White",
			"desc":"heating is complete"
		},
		{
			"code": 140,
			"bgColor": "White",
			"desc": "Address recording completed successfully"
		},
		{
			"code": 141,
			"bgColor": "White",
			"desc": "error: invalid address written to device"
		},
		{
			"code": 142,
			"bgColor": "HotPink",
			"desc": "the input of the MKV module is closed"
		},
		{
			"code": 143,
			"bgColor": "White",
			"desc": "error: MKV module input interruption"
		},
		{
			"code": 144,
			"bgColor": "White",
			"desc": "error: short circuit of MKV module input"
		},
		{
			"code": 145,
			"bgColor": "White",
			"desc": "KL is in Normal state"
		},
		{
			"code": 146,
			"bgColor": "White",
			"desc": "error: ionistors are discharged"
		},
		{
			"code": 147,
			"bgColor": "White",
			"desc": "charging of ionistors is complete"
		},
		{
			"code": 148,
			"bgColor": "Blue",
			"fgColor": "White",
			"desc": "the sprinkler opened"
		},
		{
			"code": 149,
			"bgColor": "White",
			"desc": "Module output disabled"
		},
		{
			"code": 150,
			"bgColor": "HotPink",
			"desc": "module output enabled"
		},
		{
			"code": 151,
			"bgColor": "White",
			"desc": "Open circuit or short circuit in the control circuits of the opto-relay of the output of the MK module"
		},
		{
			"code": 152,
			"bgColor": "White",
			"desc": "unspecified malfunction of the MKR module output opto-relay"
		},
		{
			"code": 153,
			"bgColor": "Red",
			"desc": "IPR button pressed"
		},
		{
			"code": 154,
			"bgColor": "White",
			"desc": "IPR button is released"
		},
		{
			"code": 155,
			"bgColor": "Red",
			"desc": "UDP button pressed"
		},
		{
			"code": 156,
			"bgColor": "White",
			"desc": "UDP or IPR-V error (the button was pressed while the cover was closed)"
		},
		{
			"code": 157,
			"bgColor": "White",
			"desc": "opened the cover of the UDP or IPR-V"
		},
		{
			"code": 158,
			"bgColor": "White",
			"desc": "closed the cover of the UDP or IPR-V"
		},
		{
			"code": 159,
			"bgColor": "White",
			"desc": "UDP button is released"
		},
		{
			"code": 165,
			"bgColor": "Aqua",
			"desc": "error: ionistors are overcharged (the voltage on them exceeded 8.1 V)"
		},
		{
			"code": 170,
			"bgColor": "Aqua",
			"desc": "error: IR LED is faulty"
		},
		{
			"code": 171,
			"bgColor": "White",
			"desc": "initialization complete"
		},
		{
			"code": 180,
			"bgColor": "White",
			"desc": "error: threshold temperature not set, default temperature set to 55 degrees"
		},
		{
			"code": 181,
			"bgColor": "Lavender",
			"desc": "a command to start the sprinkler has been received in the command buffer"
		},
		{
			"code": 182,
			"bgColor": "Lavender",
			"desc": "error: the command to start the sprinkler did not enter the command buffer"
		},
		{
			"code": 183,
			"bgColor": "White",
			"desc": "error: the command cannot be executed - the AD type is not correct"
		},
		{
			"code": 184,
			"bgColor": "White",
			"desc": "error: the command cannot be executed - the ionistors are discharged"
		},
		{
			"code": 185,
			"bgColor": "White",
			"desc": "error: the command cannot be executed - the heater is faulty"
		},
		{
			"code": 186,
			"bgColor": "White",
			"desc": "error: the command cannot be executed - there is no connection with the device"
		},
		{
			"code": 187,
			"bgColor": "White",
			"desc": "error: the command cannot be executed - the sprinkler is open"
		},
		{
			"code": 188,
			"bgColor": "White",
			"desc": "error: the command cannot be executed - the ionistors are faulty"
		},
		{
			"code": 189,
			"bgColor": "Khaki",
			"desc": "error: heating is complete, but the sprinkler has not opened"
		},
		{
			"code": 190,
			"bgColor": "chartreuse",
			"fgColor": "darkmagenta",
			"desc": "The heater has moved from the \"Failure\" or 'Opening' state to the <Normal> state",
			"addDesc": 1,
			"addDescPrefix": "Heater was previously able to ",
			"addDescPostfix": ""
		},
		{
			"code": 191,
			"bgColor": "White",
			"desc": "Heater has moved from the Malfunction or Opening state to the Normal state"
		},
		{
			"code": 192,
			"bgColor": "White",
			"desc": "the sensor has moved from the \"Malfunction\" state to the Normal state"
		},
		{
			"code": 193,
			"bgColor": "White",
			"desc": "Pre-alarm - 80% of threshold temperature"
		},
		{
			"code": 194,
			"bgColor": "White",
			"desc": "the input of the MKV module is open"
		},
		{
			"code": 195,
			"bgColor": "White",
			"desc": "Preamble transmitted successfully"
		},
		{
			"code": 196,
			"bgColor": "White",
			"desc": "error: photo path is faulty"
		},
		{
			"code": 197,
			"bgColor": "White",
			"desc": "the photo path has moved from the Malfunction state to the Normal state"
		},
		{
			"code": 198,
			"bgColor": "Gold",
			"desc": "critical dust level, IPD maintenance is required"
		},
		{
			"code": 199,
			"bgColor": "Gold",
			"desc": "maximum dust threshold, detector is not operational"
		},
		{
			"code": 200,
			"bgColor": "Gold",
			"desc": "the smoke chamber has been cleared, the re-initialization of the IPD has begun"
		},
		{
			"code": 201,
			"bgColor": "White",
			"desc": "valve in intermediate position"
		},
		{
			"code": 202,
			"bgColor": "White",
			"desc": "the valve is open"
		},
		{
			"code": 203,
			"bgColor": "White",
			"desc": "the valve is closed"
		},
		{
			"code": 204,
			"bgColor": "White",
			"desc": "open or short circuit in the valve control circuit"
		},
		{
			"code": 205,
			"bgColor": "White",
			"desc": "error: Line interruption"
		},
		{
			"code": 206,
			"bgColor": "White",
			"desc": "error: Line short circuit"
		},
		{
			"code": 207,
			"bgColor": "White",
			"desc": "Line has recovered from a malfunction"
		},
		{
			"code": 208,
			"bgColor": "White",
			"desc": "no line power"
		},
		{
			"code": 209,
			"bgColor": "White",
			"desc": "The MKV-O(S) warning line operates in straight polarity mode with blanking"
		},
		{
			"code": 210,
			"bgColor": "White",
			"desc": "The MKV-O(S) warning line operates in reverse polarity mode with blanking"
		},
		{
			"code": 211,
			"bgColor": "White",
			"desc": "MKV-O(S) warning line operates in reverse polarity mode"
		},
		{
			"code": 212,
			"bgColor": "White",
			"desc": "The MKV-O(S) warning line operates in straight polarity mode"
		},
		{
			"code": 214,
			"bgColor": "White",
			"desc": "Device firmware was successfully installed"
		},
		{
			"code": 215,
			"bgColor": "White",
			"desc": "error: firmware transfer interrupted"
		},
		{
			"code": 216,
			"bgColor": "White",
			"desc": "the preamble was transferred successfully, the process of transferring the firmware has begun"
		},
		{
			"code": 217,
			"bgColor": "White",
			"desc": "The firmware has been transferred, the CRC is being checked"
		},
		{
			"code": 218,
			"bgColor": "White",
			"desc": "error: packet retransmission"
		},
		{
			"code": 219,
			"bgColor": "White",
			"desc": "error: the firmware was transferred with an error - the CRC did not match"
		},
		{
			"code": 220,
			"bgColor": "White",
			"desc": "The firmware was transferred successfully (transferred after the firmware is transferred from an external program to the internal memory of the cable)"
		},
		{
			"code": 221,
			"bgColor": "White",
			"desc": "laser off"
		},	
		{
			"code": 222,
			"bgColor": "White",
			"desc": "laser off"
		}
	]
}
